Static Call Graph - [..\OBJ\PT100 DEMO V0.2]

# Static Call Graph for image ..\OBJ\PT100 DEMO V0.2

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Sat Sep 19 16:01:38 2020

### Maximum Stack Usage = 1088 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ Oled_Main_Task ⇒ ADL5513_dBm_Out ⇒ Get_Adc_Rms ⇒ pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC3_IRQHandler ⇒ ADC3_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from adc.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - IsKeyDownENT from matrix_key.o(.text) referenced from matrix_key.o(.text)
  - IsKeyDownS1 from matrix_key.o(.text) referenced from matrix_key.o(.text)
  - IsKeyDownS2 from matrix_key.o(.text) referenced from matrix_key.o(.text)
  - IsKeyDownS3 from matrix_key.o(.text) referenced from matrix_key.o(.text)
  - IsKeyDownS4 from matrix_key.o(.text) referenced from matrix_key.o(.text)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from timer.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - _get_lc_ctype from lc_ctype_c.o(locale$$code) referenced from rt_ctype_table.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - _sbackspace from _sgetc.o(.text) referenced from strtod.o(.text)
  - _sgetc from _sgetc.o(.text) referenced from strtod.o(.text)
  - _sputc from _sputc.o(.text) referenced from noretval__2sprintf.o(.text)
  - fputc from usart.o(.text) referenced from _printf_char_file.o(.text)
  - isspace from isspace.o(.text) referenced from strtod.o(.text)
  - mem_init from malloc.o(.text) referenced 2 times from malloc.o(.data)
  - mem_perused from malloc.o(.text) referenced 2 times from malloc.o(.data)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 90 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __decompress1 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(!!dczerorl2), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_f (Thumb, 0 bytes, Stack size unknown bytes, _printf_f.o(.ARM.Collect$$_printf_percent$$00000003))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_f ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_ll (Thumb, 0 bytes, Stack size unknown bytes, _printf_ll.o(.ARM.Collect$$_printf_percent$$00000007))

  _printf_u (Thumb, 0 bytes, Stack size unknown bytes, _printf_u.o(.ARM.Collect$$_printf_percent$$0000000A))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_u ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_llu (Thumb, 0 bytes, Stack size unknown bytes, _printf_llu.o(.ARM.Collect$$_printf_percent$$0000000F))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_llu ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_common (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))
  [Calls]

  - >> __rt_locale

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000012))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_ctype_2 ⇒ _get_lc_ctype
  [Calls]
  - >> _get_lc_ctype

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000016))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_numeric_2 ⇒ _get_lc_numeric
  [Calls]
  - >> _get_lc_numeric

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 1088 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ Oled_Main_Task ⇒ ADL5513_dBm_Out ⇒ Get_Adc_Rms ⇒ pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  main (Thumb, 762 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 1088 + Unknown Stack Size
  - Call Chain = main ⇒ Oled_Main_Task ⇒ ADL5513_dBm_Out ⇒ Get_Adc_Rms ⇒ pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> bsp_init
  - >> bsp_GetKey
  - >> bsp_ClearKey
  - >> _EC11_Spin_LableSel_Process
  - >> _EC11_Spin_LableSel_Count
  - >> _EC11_Spin_Edit_Process
  - >> _EC11_Spin_Edit_Count
  - >> _EC11_Spin_EditSel_Process
  - >> _EC11_Spin_EditSel_Count
  - >> TIM_GetCounter
  - >> TIM_Cmd
  - >> PLL_Out_Ctr
  - >> PLL_Out_Amp
  - >> Oled_Main_Task
  - >> Key_Scan_Process
  - >> CH2_Freq_Set
  - >> Amp_ASC_to_Value
  - >> __2printf
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __aeabi_cfcmpeq
  - >> __aeabi_f2d
  [Called By]
  - >> __rt_entry_main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  LED_Init (Thumb, 92 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  Adc_Init (Thumb, 202 bytes, Stack size 32 bytes, adc.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Adc_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_ADCCLKConfig
  - >> NVIC_Init
  - >> ADC_TempSensorVrefintCmd
  - >> ADC_StartCalibration
  - >> ADC_SoftwareStartConvCmd
  - >> ADC_ResetCalibration
  - >> ADC_RegularChannelConfig
  - >> ADC_Init
  - >> ADC_ITConfig
  - >> ADC_GetResetCalibrationStatus
  - >> ADC_GetCalibrationStatus
  - >> ADC_DeInit
  - >> ADC_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  Get_Adc (Thumb, 46 bytes, Stack size 8 bytes, adc.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Get_Adc ⇒ ADC_RegularChannelConfig
  [Calls]
  - >> ADC_SoftwareStartConvCmd
  - >> ADC_RegularChannelConfig
  - >> ADC_GetFlagStatus
  - >> ADC_GetConversionValue
  [Called By]
  - >> Get_Adc_LPF
  - >> Get_Adc_Rms
  - >> Get_Adc_Average

  Get_Adc_Average (Thumb, 42 bytes, Stack size 24 bytes, adc.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Get_Adc_Average ⇒ Get_Adc ⇒ ADC_RegularChannelConfig
  [Calls]
  - >> Get_Adc
  [Called By]
  - >> ADL5513_dBm_Out

  Get_Adc_Rms (Thumb, 140 bytes, Stack size 848 bytes, adc.o(.text))
  [Stack]

  - Max Depth = 1040
  - Call Chain = Get_Adc_Rms ⇒ pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> Get_Adc
  - >> sqrt
  - >> pow
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  [Called By]
  - >> ADL5513_dBm_Out

  Get_Adc_LPF (Thumb, 114 bytes, Stack size 64 bytes, adc.o(.text), UNUSED)
  [Calls]

  - >> Get_Adc
  - >> __aeabi_dmul
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> __aeabi_dsub
  - >> __aeabi_dadd

  ADC1_2_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, adc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC1_2_IRQHandler
  [Calls]
  - >> ADC_GetFlagStatus
  - >> ADC_GetConversionValue
  - >> ADC_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM3_Int_Init (Thumb, 88 bytes, Stack size 32 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM3_Int_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> TIM_Cmd
  [Called By]
  - >> bsp_init

  TIM2_Int_Init (Thumb, 92 bytes, Stack size 32 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM2_Int_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> TIM_Cmd
  [Called By]
  - >> bsp_init

  TIM5_Int_Init (Thumb, 88 bytes, Stack size 32 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM5_Int_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> TIM_Cmd
  [Called By]
  - >> bsp_init

  TIM6_Int_Init (Thumb, 88 bytes, Stack size 32 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TIM6_Int_Init ⇒ NVIC_Init
  [Calls]
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  - >> TIM_Cmd
  [Called By]
  - >> bsp_init

  TIM8_Init (Thumb, 116 bytes, Stack size 32 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = TIM8_Init ⇒ TIM_ICInit ⇒ TI1_Config
  [Calls]
  - >> TIM_TimeBaseStructInit
  - >> TIM_TimeBaseInit
  - >> TIM_ICStructInit
  - >> TIM_ICInit
  - >> TIM_EncoderInterfaceConfig
  - >> TIM_DeInit
  - >> TIM_ClearFlag
  - >> RCC_APB2PeriphClockCmd
  - >> TIM_Cmd
  [Called By]
  - >> bsp_init

  TIM3_IRQHandler (Thumb, 78 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM3_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 44 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM2_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 22 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM6_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 36 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TIM5_IRQHandler ⇒ bsp_KeyScan ⇒ bsp_DetectKey
  [Calls]
  - >> bsp_KeyScan
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, timer.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM8_UP_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  bsp_InitEC11Hard (Thumb, 66 bytes, Stack size 8 bytes, bsp_ec11.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = bsp_InitEC11Hard ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  SPI2_Init (Thumb, 124 bytes, Stack size 32 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> AD9912_HSTL_Set
  - >> AD9912_Default_Config
  - >> AD9912_CMOS_Set
  - >> AD9912_Power_Ctr
  - >> AD9912_Soft_RESET
  - >> AD9912_Read_Part_ID

  SPI2_WriteByte (Thumb, 44 bytes, Stack size 16 bytes, spi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI2_WriteByte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> AD9912_SetFreq_Hz
  - >> AD9912_SetPhase_Test
  - >> AD9912_SetFreq_Test
  - >> AD9912_SetPhase
  - >> AD9912_SetFreq
  - >> AD9912_Default_Phase_config
  - >> AD9912_Default_FTW_config

  SPI2_ReadByte (Thumb, 40 bytes, Stack size 8 bytes, spi.o(.text), UNUSED)
  [Calls]

  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus

  SPI2_ReadWriteByte (Thumb, 78 bytes, Stack size 16 bytes, spi.o(.text), UNUSED)
  [Calls]

  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus

  SPI2_ReadTwoByte (Thumb, 44 bytes, Stack size 16 bytes, spi.o(.text), UNUSED)
  [Calls]

  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus

  SPI2_WriteTwoByte (Thumb, 44 bytes, Stack size 16 bytes, spi.o(.text), UNUSED)
  [Calls]

  - >> SPI_I2S_SendData
  - >> SPI_I2S_GetFlagStatus

  OLED_WR_Byte (Thumb, 108 bytes, Stack size 16 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = OLED_WR_Byte
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> Con_4_byte
  - >> Show_Pattern
  - >> Fill_Block
  - >> Fill_Part_RAM
  - >> Set_Linear_Gray_Scale_Table
  - >> Set_Gray_Scale_Table
  - >> Set_Master_Current
  - >> Set_Start_Line
  - >> Set_Display_Offset
  - >> Set_Partial_Display
  - >> Set_Remap_Format
  - >> Set_Read_RAM
  - >> OLED_Init
  - >> Fill_RAM
  - >> Draw_Rectangle
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM

  Set_Write_RAM (Thumb, 12 bytes, Stack size 8 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Set_Write_RAM ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> Asc12_24_advant
  - >> Asc5_8_Single
  - >> Asc5_8_advant
  - >> Asc5_8
  - >> Show_Pattern
  - >> Fill_Block
  - >> Fill_Part_RAM
  - >> Fill_RAM
  - >> Draw_Rectangle

  Set_Row_Address (Thumb, 32 bytes, Stack size 16 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Set_Row_Address ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> Asc12_24_advant
  - >> Asc5_8_Single
  - >> Asc5_8_advant
  - >> Asc5_8
  - >> Show_Pattern
  - >> Fill_Block
  - >> Fill_Part_RAM
  - >> Fill_RAM
  - >> Draw_Rectangle

  Set_Column_Address (Thumb, 32 bytes, Stack size 16 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Set_Column_Address ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> Asc12_24_advant
  - >> Asc5_8_Single
  - >> Asc5_8_advant
  - >> Asc5_8
  - >> Show_Pattern
  - >> Fill_Block
  - >> Fill_Part_RAM
  - >> Fill_RAM
  - >> Draw_Rectangle

  Draw_Rectangle (Thumb, 632 bytes, Stack size 56 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Draw_Rectangle ⇒ Set_Column_Address ⇒ OLED_WR_Byte
  [Calls]
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  - >> OLED_WR_Byte
  [Called By]
  - >> OLED_Init
  - >> Oled_Main_Task
  - >> Power_menu_Fix_Display
  - >> CW_menu_Fix_Display

  Fill_RAM (Thumb, 66 bytes, Stack size 16 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Fill_RAM ⇒ Set_Column_Address ⇒ OLED_WR_Byte
  [Calls]
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  - >> OLED_WR_Byte
  [Called By]
  - >> OLED_Init
  - >> Oled_Main_Task

  OLED_Init (Thumb, 526 bytes, Stack size 16 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = OLED_Init ⇒ Draw_Rectangle ⇒ Set_Column_Address ⇒ OLED_WR_Byte
  [Calls]
  - >> Fill_RAM
  - >> Draw_Rectangle
  - >> OLED_WR_Byte
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  Set_Read_RAM (Thumb, 12 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte

  Set_Remap_Format (Thumb, 30 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte

  Set_Partial_Display (Thumb, 38 bytes, Stack size 16 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte
  [Called By]
  - >> Vertical_Scroll

  Set_Display_Offset (Thumb, 22 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte
  [Called By]
  - >> Vertical_Scroll

  Set_Start_Line (Thumb, 22 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte

  Set_Master_Current (Thumb, 22 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte

  Set_Gray_Scale_Table (Thumb, 140 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte

  Set_Linear_Gray_Scale_Table (Thumb, 12 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> OLED_WR_Byte

  Vertical_Scroll (Thumb, 132 bytes, Stack size 24 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> delay_us
  - >> Set_Display_Offset
  - >> Set_Partial_Display

  Fill_Part_RAM (Thumb, 182 bytes, Stack size 32 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  - >> OLED_WR_Byte

  Fill_Block (Thumb, 106 bytes, Stack size 32 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  - >> OLED_WR_Byte
  [Called By]
  - >> Grayscale

  Show_Pattern (Thumb, 116 bytes, Stack size 40 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  - >> OLED_WR_Byte

  Con_4_byte (Thumb, 174 bytes, Stack size 32 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> Asc12_24_advant
  - >> Asc5_8_Single
  - >> Asc5_8_advant
  - >> Asc5_8

  Asc5_8 (Thumb, 150 bytes, Stack size 32 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = Asc5_8 ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Con_4_byte
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  [Called By]
  - >> Device_name_Display

  Asc5_8_advant (Thumb, 184 bytes, Stack size 56 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Con_4_byte
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  [Called By]
  - >> Fun_KEY_Display
  - >> Power_menu_Fix_Display
  - >> CW_menu_Freq_Lable
  - >> CW_menu_Amp_Lable
  - >> CW_menu_Out_Lable
  - >> CW_menu_Out_Type
  - >> CW_menu_Freq_Unit_Lable
  - >> CW_menu_Amp_Unit_Lable

  Asc5_8_Single (Thumb, 120 bytes, Stack size 40 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Asc5_8_Single ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Con_4_byte
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  [Called By]
  - >> Oled_Main_Task
  - >> CW_menu_Fix_Display
  - >> CW_menu_Freq_show
  - >> CW_menu_Amp_show

  Asc12_24_advant (Thumb, 190 bytes, Stack size 40 bytes, oled.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Asc12_24_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Con_4_byte
  - >> Set_Column_Address
  - >> Set_Row_Address
  - >> Set_Write_RAM
  [Called By]
  - >> Power_menu_dBm_show

  Grayscale (Thumb, 132 bytes, Stack size 8 bytes, oled.o(.text), UNUSED)
  [Calls]

  - >> Fill_Block

  Dac1_Init (Thumb, 94 bytes, Stack size 24 bytes, dac.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Dac1_Init ⇒ GPIO_Init
  [Calls]
  - >> DAC_SetChannel1Data
  - >> DAC_Init
  - >> DAC_Cmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  Dac1_Set_Vol (Thumb, 60 bytes, Stack size 16 bytes, dac.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Dac1_Set_Vol ⇒ __aeabi_fmul
  [Calls]
  - >> DAC_SetChannel1Data
  - >> __aeabi_fmul
  - >> __aeabi_ui2f
  - >> __aeabi_f2uiz
  - >> __aeabi_fdiv
  [Called By]
  - >> bsp_init

  bsp_InitKey (Thumb, 12 bytes, Stack size 8 bytes, matrix_key.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = bsp_InitKey ⇒ bsp_InitKeyHard ⇒ GPIO_Init
  [Calls]
  - >> bsp_InitKeyHard
  - >> bsp_InitKeyVar
  [Called By]
  - >> bsp_init

  bsp_PutKey (Thumb, 28 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Called By]

  - >> bsp_DetectKey

  bsp_GetKey (Thumb, 46 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Called By]

  - >> main

  bsp_GetKey2 (Thumb, 46 bytes, Stack size 0 bytes, matrix_key.o(.text), UNUSED)

  bsp_GetKeyState (Thumb, 12 bytes, Stack size 0 bytes, matrix_key.o(.text), UNUSED)

  bsp_SetKeyParam (Thumb, 30 bytes, Stack size 8 bytes, matrix_key.o(.text), UNUSED)

  bsp_ClearKey (Thumb, 10 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Called By]

  - >> main

  bsp_KeyScan (Thumb, 22 bytes, Stack size 8 bytes, matrix_key.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = bsp_KeyScan ⇒ bsp_DetectKey
  [Calls]
  - >> bsp_DetectKey
  [Called By]
  - >> TIM5_IRQHandler

  PLL_Freq_Amp_Init (Thumb, 46 bytes, Stack size 8 bytes, bsp.o(.text))
  [Stack]

  - Max Depth = 264 + Unknown Stack Size
  - Call Chain = PLL_Freq_Amp_Init ⇒ CH2_Freq_Set ⇒ Set_LMX2592_Freq_RealTime ⇒ LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> LO_LMX2592_Init_Config
  - >> Freq_Value_to_ASCII_PLL
  - >> CW_Menu_Parameters_Init
  - >> PLL_Out_Amp
  - >> CH2_Freq_Set
  [Called By]
  - >> Key_S3_Down_Process
  - >> bsp_init

  bsp_init (Thumb, 194 bytes, Stack size 8 bytes, bsp.o(.text))
  [Stack]

  - Max Depth = 272 + Unknown Stack Size
  - Call Chain = bsp_init ⇒ PLL_Freq_Amp_Init ⇒ CH2_Freq_Set ⇒ Set_LMX2592_Freq_RealTime ⇒ LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> uart_init
  - >> mem_init
  - >> delay_ms
  - >> delay_init
  - >> Soft_SPI_Read_Reg
  - >> Soft_SPI_Init
  - >> PE4302_GPIO_Init
  - >> NVIC_PriorityGroupConfig
  - >> Main_menu_Win
  - >> LO_LMX2582_Init_Config
  - >> HMC241_GPIO_Init
  - >> AD9912_GPIO_init
  - >> AD9912_Default_Config
  - >> PLL_Freq_Amp_Init
  - >> bsp_InitKey
  - >> Dac1_Set_Vol
  - >> Dac1_Init
  - >> OLED_Init
  - >> bsp_InitEC11Hard
  - >> TIM8_Init
  - >> TIM6_Int_Init
  - >> TIM5_Int_Init
  - >> TIM2_Int_Init
  - >> TIM3_Int_Init
  - >> Adc_Init
  - >> LED_Init
  - >> __2printf
  [Called By]
  - >> main

  DDS_Freq_Amp_Init (Thumb, 88 bytes, Stack size 8 bytes, bsp.o(.text), UNUSED)
  [Calls]

  - >> Freq_Value_to_ASCII
  - >> Amp_Value_to_ASCII
  - >> AD9912_SetFreq_Hz
  - >> AD9912_HSTL_Set
  - >> AD9912_CMOS_Set

  Key_Scan_Process (Thumb, 228 bytes, Stack size 8 bytes, key_scan.o(.text))
  [Stack]

  - Max Depth = 280 + Unknown Stack Size
  - Call Chain = Key_Scan_Process ⇒ Key_S3_Down_Process ⇒ PLL_Freq_Amp_Init ⇒ CH2_Freq_Set ⇒ Set_LMX2592_Freq_RealTime ⇒ LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Key_S3_Down_Process
  - >> Key_S2_Down_Process
  - >> Key_S1_Down_Process_Other
  - >> EC11_Key_LONG
  - >> EC11_Key_Down
  - >> __2printf
  [Called By]
  - >> main

  delay_init (Thumb, 50 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> bsp_init

  delay_us (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> Soft_SPI_Read_Reg
  - >> AD9912_SetFreq_Hz
  - >> Vertical_Scroll
  - >> PE4302_Set
  - >> AD9912_IO_update
  - >> AD9912_Soft_ReadByte
  - >> AD9912_Soft_WriteByte
  - >> Soft_SPI_WriteByte

  delay_ms (Thumb, 72 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> LO_LMX2592_Init_Config
  - >> LO_LMX2582_Init_Config
  - >> AD9912_GPIO_init
  - >> bsp_init
  - >> AD9912_SetPhase_Test
  - >> AD9912_SetFreq_Test
  - >> AD9912_SetPhase
  - >> AD9912_SetFreq
  - >> AD9912_Default_Phase_config
  - >> AD9912_Default_FTW_config
  - >> AD9912_Soft_Clear_UPDATE
  - >> AD9912_Soft_UPDATE
  - >> AD9912_Soft_RESET
  - >> ALL_PLL_Init

  _sys_exit (Thumb, 6 bytes, Stack size 0 bytes, usart.o(.text))
  [Called By]

  - >> __rt_exit_exit

  fputc (Thumb, 24 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - _printf_char_file.o(.text)

  uart_init (Thumb, 154 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC3_IRQHandler
  [Called By]
  - >> ADC3_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  Fun_KEY_Display (Thumb, 234 bytes, Stack size 16 bytes, main_menu.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = Fun_KEY_Display ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> Main_menu_Win
  - >> Oled_Main_Task
  - >> Power_menu_Win
  - >> CW_Menu_Read_Only_Win

  Device_name_Display (Thumb, 14 bytes, Stack size 8 bytes, main_menu.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Device_name_Display ⇒ Asc5_8 ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8
  [Called By]
  - >> Main_menu_Win

  Main_menu_Win (Thumb, 14 bytes, Stack size 8 bytes, main_menu.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = Main_menu_Win ⇒ Fun_KEY_Display ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Device_name_Display
  - >> Fun_KEY_Display
  [Called By]
  - >> bsp_init
  - >> Oled_Main_Task

  CW_Menu_Parameters_Init (Thumb, 44 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = CW_Menu_Parameters_Init ⇒ Amp_Value_to_ASCII ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Amp_Value_to_ASCII
  [Called By]
  - >> PLL_Freq_Amp_Init

  CW_menu_Amp_Unit_Lable (Thumb, 18 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CW_menu_Amp_Unit_Lable ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> CW_Menu_Read_Only_Win

  CW_menu_Freq_Unit_Lable (Thumb, 84 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CW_menu_Freq_Unit_Lable ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> CW_Menu_Edit_Select_Win
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_menu_Out_Type (Thumb, 100 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CW_menu_Out_Type ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> CW_Menu_Edit_Select_Win
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_menu_Amp_show (Thumb, 170 bytes, Stack size 16 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = CW_menu_Amp_show ⇒ Asc5_8_Single ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_Single
  [Called By]
  - >> CW_menu_Win
  - >> CW_Menu_Edit_Select_Win
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_menu_Freq_show (Thumb, 184 bytes, Stack size 16 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = CW_menu_Freq_show ⇒ Asc5_8_Single ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_Single
  [Called By]
  - >> CW_menu_Win
  - >> CW_Menu_Edit_Select_Win
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_menu_Out_Lable (Thumb, 18 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CW_menu_Out_Lable ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_menu_Amp_Lable (Thumb, 18 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CW_menu_Amp_Lable ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_menu_Freq_Lable (Thumb, 18 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CW_menu_Freq_Lable ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  [Called By]
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win

  CW_Menu_Read_Only_Win (Thumb, 58 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = CW_Menu_Read_Only_Win ⇒ Fun_KEY_Display ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Fun_KEY_Display
  - >> CW_menu_Freq_Lable
  - >> CW_menu_Amp_Lable
  - >> CW_menu_Out_Lable
  - >> CW_menu_Freq_show
  - >> CW_menu_Amp_show
  - >> CW_menu_Out_Type
  - >> CW_menu_Freq_Unit_Lable
  - >> CW_menu_Amp_Unit_Lable
  [Called By]
  - >> CW_menu_Win

  CW_Menu_Lable_Select_Win (Thumb, 174 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = CW_Menu_Lable_Select_Win ⇒ CW_menu_Freq_Lable ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> CW_menu_Freq_Lable
  - >> CW_menu_Amp_Lable
  - >> CW_menu_Out_Lable
  - >> CW_menu_Freq_show
  - >> CW_menu_Amp_show
  - >> CW_menu_Out_Type
  - >> CW_menu_Freq_Unit_Lable
  [Called By]
  - >> CW_menu_Win

  CW_Menu_Edit_Select_Win (Thumb, 60 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = CW_Menu_Edit_Select_Win ⇒ CW_menu_Out_Type ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> CW_menu_Freq_show
  - >> CW_menu_Amp_show
  - >> CW_menu_Out_Type
  - >> CW_menu_Freq_Unit_Lable
  [Called By]
  - >> CW_menu_Win

  CW_menu_Fix_Display (Thumb, 216 bytes, Stack size 16 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = CW_menu_Fix_Display ⇒ Asc5_8_Single ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_Single
  - >> Draw_Rectangle
  [Called By]
  - >> CW_menu_Win

  CW_menu_Win (Thumb, 96 bytes, Stack size 8 bytes, cw_menu.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = CW_menu_Win ⇒ CW_Menu_Read_Only_Win ⇒ Fun_KEY_Display ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> CW_menu_Fix_Display
  - >> CW_Menu_Edit_Select_Win
  - >> CW_Menu_Lable_Select_Win
  - >> CW_Menu_Read_Only_Win
  - >> CW_menu_Freq_show
  - >> CW_menu_Amp_show
  [Called By]
  - >> Oled_Main_Task

  Power_menu_dBm_show (Thumb, 106 bytes, Stack size 24 bytes, power_menu.o(.text))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = Power_menu_dBm_show ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Asc12_24_advant
  - >> __2sprintf
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __aeabi_f2d
  [Called By]
  - >> Oled_Main_Task
  - >> Power_menu_Win

  Power_menu_Fix_Display (Thumb, 52 bytes, Stack size 16 bytes, power_menu.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = Power_menu_Fix_Display ⇒ Asc5_8_advant ⇒ Con_4_byte ⇒ OLED_WR_Byte
  [Calls]
  - >> Asc5_8_advant
  - >> Draw_Rectangle
  [Called By]
  - >> Power_menu_Win

  Power_menu_Win (Thumb, 38 bytes, Stack size 8 bytes, power_menu.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = Power_menu_Win ⇒ Power_menu_dBm_show ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Fun_KEY_Display
  - >> Power_menu_Fix_Display
  - >> Power_menu_dBm_show
  [Called By]
  - >> Oled_Main_Task

  Oled_Main_Task (Thumb, 226 bytes, Stack size 16 bytes, oled_task.o(.text))
  [Stack]

  - Max Depth = 1088 + Unknown Stack Size
  - Call Chain = Oled_Main_Task ⇒ ADL5513_dBm_Out ⇒ Get_Adc_Rms ⇒ pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> Fun_KEY_Display
  - >> Main_menu_Win
  - >> Asc5_8_Single
  - >> Fill_RAM
  - >> Draw_Rectangle
  - >> ADL5513_dBm_Out
  - >> Power_menu_Win
  - >> Power_menu_dBm_show
  - >> CW_menu_Win
  - >> __aeabi_cfcmpeq
  [Called By]
  - >> main

  Key_S1_Down_Process_Other (Thumb, 76 bytes, Stack size 0 bytes, key_s1_process.o(.text))
  [Called By]

  - >> Key_Scan_Process

  Key_S2_Down_Process (Thumb, 4 bytes, Stack size 0 bytes, key_s2_process.o(.text))
  [Called By]

  - >> Key_Scan_Process

  Key_S3_Down_Process (Thumb, 124 bytes, Stack size 8 bytes, key_s3_process.o(.text))
  [Stack]

  - Max Depth = 272 + Unknown Stack Size
  - Call Chain = Key_S3_Down_Process ⇒ PLL_Freq_Amp_Init ⇒ CH2_Freq_Set ⇒ Set_LMX2592_Freq_RealTime ⇒ LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> PLL_Freq_Amp_Init
  [Called By]
  - >> Key_Scan_Process

  EC11_Key_Down (Thumb, 108 bytes, Stack size 0 bytes, ec11_key_process.o(.text))
  [Called By]

  - >> Key_Scan_Process

  EC11_Key_LONG (Thumb, 50 bytes, Stack size 0 bytes, ec11_key_process.o(.text))
  [Called By]

  - >> Key_Scan_Process

  _EC11_Spin_LableSel_Count (Thumb, 84 bytes, Stack size 0 bytes, ec11_spin_process.o(.text))
  [Called By]

  - >> main

  _EC11_Spin_LableSel_Process (Thumb, 76 bytes, Stack size 0 bytes, ec11_spin_process.o(.text))
  [Called By]

  - >> main

  _EC11_Spin_EditSel_Count (Thumb, 84 bytes, Stack size 0 bytes, ec11_spin_process.o(.text))
  [Called By]

  - >> main

  _EC11_Spin_EditSel_Process (Thumb, 484 bytes, Stack size 0 bytes, ec11_spin_process.o(.text))
  [Called By]

  - >> main

  _EC11_Spin_Edit_Count (Thumb, 84 bytes, Stack size 0 bytes, ec11_spin_process.o(.text))
  [Called By]

  - >> main

  _EC11_Amp_Step_Up (Thumb, 154 bytes, Stack size 8 bytes, ec11_spin_process.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = _EC11_Amp_Step_Up ⇒ Amp_ASC_to_Value ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> Amp_Value_to_ASCII
  - >> Amp_ASC_to_Value
  - >> __2printf
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __aeabi_fadd
  [Called By]
  - >> _EC11_Spin_Edit_Process

  _EC11_Freq_Step_Up (Thumb, 778 bytes, Stack size 16 bytes, ec11_spin_process.o(.text))
  [Stack]

  - Max Depth = 504 + Unknown Stack Size
  - Call Chain = _EC11_Freq_Step_Up ⇒ Freq_ASC_to_Value_PLL ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> Freq_Value_to_ASCII_PLL
  - >> Freq_Value_to_ASCII
  - >> __2printf
  - >> Freq_ASC_to_Value_PLL
  - >> Freq_ASC_to_Value
  [Called By]
  - >> _EC11_Spin_Edit_Process

  _EC11_Amp_Step_Down (Thumb, 158 bytes, Stack size 8 bytes, ec11_spin_process.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = _EC11_Amp_Step_Down ⇒ Amp_ASC_to_Value ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> Amp_Value_to_ASCII
  - >> Amp_ASC_to_Value
  - >> __2printf
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __aeabi_fsub
  [Called By]
  - >> _EC11_Spin_Edit_Process

  _EC11_Freq_Step_Down (Thumb, 976 bytes, Stack size 16 bytes, ec11_spin_process.o(.text))
  [Stack]

  - Max Depth = 504 + Unknown Stack Size
  - Call Chain = _EC11_Freq_Step_Down ⇒ Freq_ASC_to_Value_PLL ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> Freq_Value_to_ASCII_PLL
  - >> Freq_Value_to_ASCII
  - >> __2printf
  - >> Freq_ASC_to_Value_PLL
  - >> Freq_ASC_to_Value
  [Called By]
  - >> _EC11_Spin_Edit_Process

  _EC11_Spin_Edit_Process (Thumb, 76 bytes, Stack size 8 bytes, ec11_spin_process.o(.text))
  [Stack]

  - Max Depth = 512 + Unknown Stack Size
  - Call Chain = _EC11_Spin_Edit_Process ⇒ _EC11_Freq_Step_Down ⇒ Freq_ASC_to_Value_PLL ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _EC11_Freq_Step_Down
  - >> _EC11_Amp_Step_Down
  - >> _EC11_Freq_Step_Up
  - >> _EC11_Amp_Step_Up
  [Called By]
  - >> main

  Soft_SPI_Init (Thumb, 124 bytes, Stack size 8 bytes, pll_spi_init.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Soft_SPI_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> bsp_init
  - >> ALL_PLL_Init

  Soft_SPI_WriteByte (Thumb, 218 bytes, Stack size 24 bytes, pll_spi_init.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_us
  - >> __2printf
  [Called By]
  - >> LO_LMX2592_Init_Config
  - >> LO_LMX2582_Init_Config
  - >> PLL_Out_Ctr
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO

  Soft_SPI_Read_Reg (Thumb, 348 bytes, Stack size 24 bytes, pll_spi_init.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = Soft_SPI_Read_Reg ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_us
  - >> __2printf
  [Called By]
  - >> bsp_init

  LO_LMX2582_Init_Config (Thumb, 70 bytes, Stack size 8 bytes, all_lo_init.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = LO_LMX2582_Init_Config ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> Soft_SPI_WriteByte
  [Called By]
  - >> bsp_init
  - >> ALL_PLL_Init

  ALL_PLL_Init (Thumb, 30 bytes, Stack size 8 bytes, all_lo_init.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> Soft_SPI_Init
  - >> LO_LMX2582_Init_Config

  PLL_Out_Ctr (Thumb, 178 bytes, Stack size 16 bytes, all_lo_init.o(.text))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = PLL_Out_Ctr ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  - >> Soft_SPI_WriteByte
  [Called By]
  - >> main

  LO_LMX2592_Init_Config (Thumb, 104 bytes, Stack size 8 bytes, all_lo_init.o(.text))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = LO_LMX2592_Init_Config ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> delay_ms
  - >> Soft_SPI_WriteByte
  [Called By]
  - >> PLL_Freq_Amp_Init

  LMX2592_OUT_VCO (Thumb, 268 bytes, Stack size 32 bytes, lo_lmx2592_freq_set.o(.text))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = LMX2592_OUT_VCO ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> AD9912_SetFreq_Hz
  - >> Soft_SPI_WriteByte
  - >> __aeabi_dmul
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> __aeabi_ddiv
  [Called By]
  - >> Set_LMX2592_Freq_RealTime

  LMX2592_OUT_DIV (Thumb, 852 bytes, Stack size 32 bytes, lo_lmx2592_freq_set.o(.text))
  [Stack]

  - Max Depth = 200 + Unknown Stack Size
  - Call Chain = LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> AD9912_SetFreq_Hz
  - >> Soft_SPI_WriteByte
  - >> __aeabi_dmul
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  - >> __aeabi_ddiv
  [Called By]
  - >> Set_LMX2592_Freq_RealTime

  LMX2592_DIV (Thumb, 466 bytes, Stack size 0 bytes, lo_lmx2592_freq_set.o(.text))
  [Called By]

  - >> Set_LMX2592_Freq_RealTime

  Set_LMX2592_Freq_RealTime (Thumb, 138 bytes, Stack size 24 bytes, lo_lmx2592_freq_set.o(.text))
  [Stack]

  - Max Depth = 224 + Unknown Stack Size
  - Call Chain = Set_LMX2592_Freq_RealTime ⇒ LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> LMX2592_DIV
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO
  - >> __aeabi_cdrcmple
  - >> __aeabi_dmul
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  [Called By]
  - >> CH2_Freq_Set

  AD9912_GPIO_init (Thumb, 80 bytes, Stack size 8 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AD9912_GPIO_init ⇒ GPIO_Init
  [Calls]
  - >> delay_ms
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> bsp_init

  AD9912_Soft_Spi_Init (Thumb, 40 bytes, Stack size 8 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = AD9912_Soft_Spi_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> AD9912_HSTL_Set
  - >> AD9912_Default_Config
  - >> AD9912_CMOS_Set
  - >> AD9912_Power_Ctr
  - >> AD9912_Soft_RESET
  - >> AD9912_Read_Part_ID

  AD9912_Soft_WriteByte (Thumb, 126 bytes, Stack size 24 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = AD9912_Soft_WriteByte ⇒ GPIO_Init
  [Calls]
  - >> delay_us
  - >> GPIO_Init
  [Called By]
  - >> AD9912_HSTL_Set
  - >> AD9912_Default_Config
  - >> AD9912_CMOS_Set
  - >> AD9912_Power_Ctr
  - >> AD9912_Soft_Clear_UPDATE
  - >> AD9912_Soft_UPDATE
  - >> AD9912_Soft_RESET

  AD9912_Soft_ReadByte (Thumb, 232 bytes, Stack size 32 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_us
  - >> GPIO_Init
  [Called By]
  - >> AD9912_HSTL_Set
  - >> AD9912_CMOS_Set
  - >> AD9912_Power_Ctr
  - >> AD9912_Read_Part_ID

  AD9912_Read_Part_ID (Thumb, 44 bytes, Stack size 8 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> SPI2_Init
  - >> AD9912_Soft_ReadByte
  - >> AD9912_Soft_Spi_Init

  AD9912_Soft_RESET (Thumb, 34 bytes, Stack size 8 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_Init
  - >> AD9912_Soft_WriteByte
  - >> AD9912_Soft_Spi_Init

  AD9912_Soft_UPDATE (Thumb, 18 bytes, Stack size 8 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = AD9912_Soft_UPDATE ⇒ AD9912_Soft_WriteByte ⇒ GPIO_Init
  [Calls]
  - >> delay_ms
  - >> AD9912_Soft_WriteByte
  [Called By]
  - >> AD9912_HSTL_Set
  - >> AD9912_Default_Config
  - >> AD9912_CMOS_Set
  - >> AD9912_Power_Ctr

  AD9912_Soft_Clear_UPDATE (Thumb, 18 bytes, Stack size 8 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = AD9912_Soft_Clear_UPDATE ⇒ AD9912_Soft_WriteByte ⇒ GPIO_Init
  [Calls]
  - >> delay_ms
  - >> AD9912_Soft_WriteByte
  [Called By]
  - >> AD9912_HSTL_Set
  - >> AD9912_Default_Config
  - >> AD9912_CMOS_Set
  - >> AD9912_Power_Ctr

  AD9912_IO_update (Thumb, 26 bytes, Stack size 8 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = AD9912_IO_update
  [Calls]
  - >> delay_us
  [Called By]
  - >> AD9912_SetFreq_Hz
  - >> AD9912_SetPhase_Test
  - >> AD9912_SetFreq_Test
  - >> AD9912_SetPhase
  - >> AD9912_SetFreq
  - >> AD9912_Default_Phase_config
  - >> AD9912_Default_FTW_config

  AD9912_Default_Config (Thumb, 72 bytes, Stack size 8 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = AD9912_Default_Config ⇒ SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> SPI2_Init
  - >> AD9912_Soft_Clear_UPDATE
  - >> AD9912_Soft_UPDATE
  - >> AD9912_Soft_WriteByte
  - >> AD9912_Soft_Spi_Init
  [Called By]
  - >> bsp_init

  AD9912_Default_FTW_config (Thumb, 74 bytes, Stack size 16 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_WriteByte
  - >> AD9912_IO_update

  AD9912_Default_Phase_config (Thumb, 74 bytes, Stack size 16 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_WriteByte
  - >> AD9912_IO_update

  AD9912_Freq_Convert (Thumb, 86 bytes, Stack size 40 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ui2d
  - >> __aeabi_d2ulz
  [Called By]
  - >> AD9912_SetFreq_Test
  - >> AD9912_SetFreq

  AD9912_Freq_Convert_Hz (Thumb, 90 bytes, Stack size 40 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = AD9912_Freq_Convert_Hz ⇒ __aeabi_dmul
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_ui2d
  - >> __aeabi_d2ulz
  [Called By]
  - >> AD9912_SetFreq_Hz

  AD9912_Phase_Convert (Thumb, 96 bytes, Stack size 32 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ui2d
  - >> __aeabi_d2uiz
  [Called By]
  - >> AD9912_SetPhase_Test
  - >> AD9912_SetPhase

  AD9912_SetFreq (Thumb, 70 bytes, Stack size 16 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_WriteByte
  - >> AD9912_Freq_Convert
  - >> AD9912_IO_update

  AD9912_SetFreq_Hz (Thumb, 70 bytes, Stack size 16 bytes, ad9912_drive.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = AD9912_SetFreq_Hz ⇒ AD9912_Freq_Convert_Hz ⇒ __aeabi_dmul
  [Calls]
  - >> delay_us
  - >> SPI2_WriteByte
  - >> AD9912_Freq_Convert_Hz
  - >> AD9912_IO_update
  [Called By]
  - >> DDS_Freq_Amp_Init
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO

  AD9912_SetPhase (Thumb, 84 bytes, Stack size 8 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_WriteByte
  - >> AD9912_Phase_Convert
  - >> AD9912_IO_update

  AD9912_SetFreq_Test (Thumb, 72 bytes, Stack size 8 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_WriteByte
  - >> AD9912_Freq_Convert
  - >> AD9912_IO_update

  AD9912_SetPhase_Test (Thumb, 84 bytes, Stack size 8 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> delay_ms
  - >> SPI2_WriteByte
  - >> AD9912_Phase_Convert
  - >> AD9912_IO_update

  AD9912_Power_Ctr (Thumb, 158 bytes, Stack size 24 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> SPI2_Init
  - >> AD9912_Soft_Clear_UPDATE
  - >> AD9912_Soft_UPDATE
  - >> AD9912_Soft_ReadByte
  - >> AD9912_Soft_WriteByte
  - >> AD9912_Soft_Spi_Init

  AD9912_HSTL_Set (Thumb, 124 bytes, Stack size 24 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> SPI2_Init
  - >> AD9912_Soft_Clear_UPDATE
  - >> AD9912_Soft_UPDATE
  - >> AD9912_Soft_ReadByte
  - >> AD9912_Soft_WriteByte
  - >> AD9912_Soft_Spi_Init
  [Called By]
  - >> DDS_Freq_Amp_Init

  AD9912_CMOS_Set (Thumb, 148 bytes, Stack size 24 bytes, ad9912_drive.o(.text), UNUSED)
  [Calls]

  - >> SPI2_Init
  - >> AD9912_Soft_Clear_UPDATE
  - >> AD9912_Soft_UPDATE
  - >> AD9912_Soft_ReadByte
  - >> AD9912_Soft_WriteByte
  - >> AD9912_Soft_Spi_Init
  [Called By]
  - >> DDS_Freq_Amp_Init

  PE4302_GPIO_Init (Thumb, 96 bytes, Stack size 8 bytes, pe4302.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = PE4302_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> GPIO_PinRemapConfig
  [Called By]
  - >> bsp_init

  PE4302_Set (Thumb, 122 bytes, Stack size 16 bytes, pe4302.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = PE4302_Set
  [Calls]
  - >> delay_us
  [Called By]
  - >> PLL_Out_Amp
  - >> DDS_Out_Amp

  HMC241_GPIO_Init (Thumb, 80 bytes, Stack size 8 bytes, hmc241.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = HMC241_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> GPIO_PinRemapConfig
  [Called By]
  - >> bsp_init

  HMC241_Set (Thumb, 122 bytes, Stack size 0 bytes, hmc241.o(.text))
  [Called By]

  - >> PLL_Out_Amp
  - >> DDS_Out_Amp

  ADL5513_dBm_Out (Thumb, 358 bytes, Stack size 32 bytes, adl5513.o(.text))
  [Stack]

  - Max Depth = 1072
  - Call Chain = ADL5513_dBm_Out ⇒ Get_Adc_Rms ⇒ pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> Get_Adc_Rms
  - >> Get_Adc_Average
  - >> __aeabi_cfrcmple
  - >> __aeabi_fmul
  - >> __aeabi_cfcmple
  - >> __aeabi_ui2f
  - >> __aeabi_fdiv
  - >> __aeabi_fsub
  - >> __aeabi_fadd
  [Called By]
  - >> Oled_Main_Task

  DDS_Out_Amp (Thumb, 580 bytes, Stack size 56 bytes, amp_set.o(.text), UNUSED)
  [Calls]

  - >> __2printf
  - >> HMC241_Set
  - >> PE4302_Set
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __aeabi_f2uiz
  - >> __aeabi_fsub
  - >> __aeabi_frsub
  - >> __aeabi_fadd
  - >> __aeabi_f2d
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ui2d
  - >> __aeabi_dadd

  PLL_Out_Amp (Thumb, 400 bytes, Stack size 24 bytes, amp_set.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = PLL_Out_Amp ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2printf
  - >> HMC241_Set
  - >> PE4302_Set
  - >> __aeabi_cfrcmple
  - >> __aeabi_cfcmple
  - >> __aeabi_f2uiz
  - >> __aeabi_frsub
  - >> __aeabi_fadd
  [Called By]
  - >> PLL_Freq_Amp_Init
  - >> main

  Amp_ASC_to_Value (Thumb, 310 bytes, Stack size 32 bytes, amp_set.o(.text))
  [Stack]

  - Max Depth = 480
  - Call Chain = Amp_ASC_to_Value ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> atof
  - >> __aeabi_d2f
  [Called By]
  - >> main
  - >> _EC11_Amp_Step_Down
  - >> _EC11_Amp_Step_Up

  Amp_Value_to_ASCII (Thumb, 54 bytes, Stack size 32 bytes, amp_set.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = Amp_Value_to_ASCII ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2sprintf
  - >> __aeabi_f2d
  [Called By]
  - >> CW_Menu_Parameters_Init
  - >> DDS_Freq_Amp_Init
  - >> _EC11_Amp_Step_Down
  - >> _EC11_Amp_Step_Up

  Freq_ASC_to_Value (Thumb, 94 bytes, Stack size 24 bytes, ch2_freq_set.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = Freq_ASC_to_Value ⇒ atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> atoi
  [Called By]
  - >> _EC11_Freq_Step_Down
  - >> _EC11_Freq_Step_Up

  Freq_ASC_to_Value_PLL (Thumb, 136 bytes, Stack size 40 bytes, ch2_freq_set.o(.text))
  [Stack]

  - Max Depth = 488
  - Call Chain = Freq_ASC_to_Value_PLL ⇒ atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> atof
  - >> __aeabi_d2ulz
  [Called By]
  - >> _EC11_Freq_Step_Down
  - >> _EC11_Freq_Step_Up

  Freq_Value_to_ASCII (Thumb, 98 bytes, Stack size 24 bytes, ch2_freq_set.o(.text))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = Freq_Value_to_ASCII ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2sprintf
  [Called By]
  - >> DDS_Freq_Amp_Init
  - >> _EC11_Freq_Step_Down
  - >> _EC11_Freq_Step_Up

  Freq_Value_to_ASCII_PLL (Thumb, 112 bytes, Stack size 32 bytes, ch2_freq_set.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = Freq_Value_to_ASCII_PLL ⇒ __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __2sprintf
  [Called By]
  - >> PLL_Freq_Amp_Init
  - >> _EC11_Freq_Step_Down
  - >> _EC11_Freq_Step_Up

  CH2_Freq_Set (Thumb, 94 bytes, Stack size 32 bytes, ch2_freq_set.o(.text))
  [Stack]

  - Max Depth = 256 + Unknown Stack Size
  - Call Chain = CH2_Freq_Set ⇒ Set_LMX2592_Freq_RealTime ⇒ LMX2592_OUT_DIV ⇒ Soft_SPI_WriteByte ⇒ __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Set_LMX2592_Freq_RealTime
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __aeabi_ul2d
  - >> __aeabi_ddiv
  [Called By]
  - >> PLL_Freq_Amp_Init
  - >> main

  mymemcpy (Thumb, 26 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Called By]

  - >> myrealloc

  mymemset (Thumb, 20 bytes, Stack size 12 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = mymemset
  [Called By]
  - >> mem_init

  mem_init (Thumb, 38 bytes, Stack size 4 bytes, malloc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = mem_init ⇒ mymemset
  [Calls]
  - >> mymemset
  [Called By]
  - >> bsp_init
  [Address Reference Count : 1]
  - malloc.o(.data)

  mem_perused (Thumb, 42 bytes, Stack size 0 bytes, malloc.o(.text))
  [Address Reference Count : 1]

  - malloc.o(.data)

  mem_malloc (Thumb, 116 bytes, Stack size 24 bytes, malloc.o(.text), UNUSED)
  [Called By]

  - >> myrealloc
  - >> mymalloc

  mem_free (Thumb, 66 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Called By]

  - >> myfree

  myfree (Thumb, 24 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Calls]

  - >> mem_free
  [Called By]
  - >> myrealloc

  mymalloc (Thumb, 28 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Calls]

  - >> mem_malloc

  myrealloc (Thumb, 50 bytes, Stack size 16 bytes, malloc.o(.text), UNUSED)
  [Calls]

  - >> myfree
  - >> mem_malloc
  - >> mymemcpy

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> uart_init
  - >> Soft_SPI_Init
  - >> PE4302_GPIO_Init
  - >> HMC241_GPIO_Init
  - >> AD9912_GPIO_init
  - >> bsp_InitKeyHard
  - >> Dac1_Init
  - >> OLED_Init
  - >> SPI2_Init
  - >> bsp_InitEC11Hard
  - >> Adc_Init
  - >> LED_Init
  - >> AD9912_Soft_ReadByte
  - >> AD9912_Soft_WriteByte
  - >> AD9912_Soft_Spi_Init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> bsp_InitKeyHard
  - >> Dac1_Init
  - >> OLED_Init
  - >> OLED_WR_Byte
  - >> LED_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> OLED_WR_Byte
  - >> LED_Init

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> PE4302_GPIO_Init
  - >> HMC241_GPIO_Init

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> Adc_Init

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> I2S_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> uart_init
  - >> Soft_SPI_Init
  - >> PE4302_GPIO_Init
  - >> HMC241_GPIO_Init
  - >> AD9912_GPIO_init
  - >> bsp_InitKeyHard
  - >> Dac1_Init
  - >> OLED_Init
  - >> SPI2_Init
  - >> bsp_InitEC11Hard
  - >> TIM8_Init
  - >> Adc_Init
  - >> LED_Init
  - >> AD9912_Soft_Spi_Init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> Dac1_Init
  - >> SPI2_Init
  - >> TIM6_Int_Init
  - >> TIM5_Int_Init
  - >> TIM2_Int_Init
  - >> TIM3_Int_Init

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> TIM_DeInit
  - >> ADC_DeInit
  - >> SPI_I2S_DeInit
  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> TIM_DeInit
  - >> DAC_DeInit
  - >> SPI_I2S_DeInit
  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> uart_init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> uart_init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> uart_init

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearITPendingBit (Thumb, 52 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> bsp_init

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> uart_init
  - >> TIM6_Int_Init
  - >> TIM5_Int_Init
  - >> TIM2_Int_Init
  - >> TIM3_Int_Init
  - >> Adc_Init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  ADC_DeInit (Thumb, 78 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DeInit
  [Calls]
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> Adc_Init

  ADC_Init (Thumb, 70 bytes, Stack size 12 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = ADC_Init
  [Called By]
  - >> Adc_Init

  ADC_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Adc_Init

  ADC_DMACmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ITConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_ITConfig
  [Called By]
  - >> Adc_Init

  ADC_ResetCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Adc_Init

  ADC_GetResetCalibrationStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Adc_Init

  ADC_StartCalibration (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Adc_Init

  ADC_GetCalibrationStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Adc_Init

  ADC_SoftwareStartConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Get_Adc
  - >> Adc_Init

  ADC_GetSoftwareStartConvStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_DiscModeChannelCountConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_DiscModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_RegularChannelConfig (Thumb, 184 bytes, Stack size 20 bytes, stm32f10x_adc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = ADC_RegularChannelConfig
  [Called By]
  - >> Get_Adc
  - >> Adc_Init

  ADC_ExternalTrigConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetConversionValue (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> ADC1_2_IRQHandler
  - >> Get_Adc

  ADC_GetDualModeConversionValue (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AutoInjectedConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_InjectedDiscModeCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ExternalTrigInjectedConvConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ExternalTrigInjectedConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_SoftwareStartInjectedConvCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetSoftwareStartInjectedConvCmdStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_InjectedChannelConfig (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_InjectedSequencerLengthConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_SetInjectedOffset (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetInjectedConversionValue (Thumb, 28 bytes, Stack size 8 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AnalogWatchdogCmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AnalogWatchdogThresholdsConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_AnalogWatchdogSingleChannelConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_TempSensorVrefintCmd (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> Adc_Init

  ADC_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> ADC1_2_IRQHandler
  - >> Get_Adc

  ADC_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_GetITStatus (Thumb, 36 bytes, Stack size 16 bytes, stm32f10x_adc.o(.text), UNUSED)

  ADC_ClearITPendingBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_adc.o(.text))
  [Called By]

  - >> ADC1_2_IRQHandler

  TIM_DeInit (Thumb, 424 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> TIM8_Init

  TIM_TimeBaseInit (Thumb, 122 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM8_Init
  - >> TIM6_Int_Init
  - >> TIM5_Int_Init
  - >> TIM2_Int_Init
  - >> TIM3_Int_Init

  TIM_OC1Init (Thumb, 132 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 154 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 150 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 182 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM_ICInit
  - >> TIM_PWMIConfig

  TIM_SetIC1Prescaler (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM_ICInit
  - >> TIM_PWMIConfig

  TIM_ICInit (Thumb, 150 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TIM_ICInit ⇒ TI1_Config
  [Calls]
  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config
  - >> TI3_Config
  - >> TI4_Config
  [Called By]
  - >> TIM8_Init

  TIM_PWMIConfig (Thumb, 124 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_BDTRConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM8_Init

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM8_Init

  TIM_BDTRStructInit (Thumb, 40 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM8_Init
  - >> TIM6_Int_Init
  - >> TIM5_Int_Init
  - >> TIM2_Int_Init
  - >> TIM3_Int_Init
  - >> main

  TIM_CtrlPWMOutputs (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM6_Int_Init
  - >> TIM5_Int_Init
  - >> TIM2_Int_Init
  - >> TIM3_Int_Init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMAConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 62 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 28 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 54 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 32 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 66 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_EncoderInterfaceConfig
  [Called By]
  - >> TIM8_Init

  TIM_ForcedOC1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 30 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 82 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOutputTrigger (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture1 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> main

  TIM_GetPrescaler (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM8_Init

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM8_UP_IRQHandler
  - >> TIM5_IRQHandler
  - >> TIM6_IRQHandler
  - >> TIM2_IRQHandler
  - >> TIM3_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM8_UP_IRQHandler
  - >> TIM5_IRQHandler
  - >> TIM6_IRQHandler
  - >> TIM2_IRQHandler
  - >> TIM3_IRQHandler

  SPI_I2S_DeInit (Thumb, 76 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI2_Init

  I2S_Init (Thumb, 226 bytes, Stack size 56 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_Init

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 32 bytes, Stack size 12 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_WriteTwoByte
  - >> SPI2_ReadWriteByte
  - >> SPI2_WriteByte

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Called By]

  - >> SPI2_ReadTwoByte
  - >> SPI2_ReadWriteByte
  - >> SPI2_ReadByte

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_WriteTwoByte
  - >> SPI2_ReadTwoByte
  - >> SPI2_ReadWriteByte
  - >> SPI2_ReadByte
  - >> SPI2_WriteByte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)

  DAC_DeInit (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_dac.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd

  DAC_Init (Thumb, 46 bytes, Stack size 12 bytes, stm32f10x_dac.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DAC_Init
  [Called By]
  - >> Dac1_Init

  DAC_StructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_Cmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f10x_dac.o(.text))
  [Called By]

  - >> Dac1_Init

  DAC_DMACmd (Thumb, 38 bytes, Stack size 0 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_SoftwareTriggerCmd (Thumb, 48 bytes, Stack size 8 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_DualSoftwareTriggerCmd (Thumb, 38 bytes, Stack size 0 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_WaveGenerationCmd (Thumb, 36 bytes, Stack size 8 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_SetChannel1Data (Thumb, 26 bytes, Stack size 8 bytes, stm32f10x_dac.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DAC_SetChannel1Data
  [Called By]
  - >> Dac1_Set_Vol
  - >> Dac1_Init

  DAC_SetChannel2Data (Thumb, 26 bytes, Stack size 8 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_SetDualChannelData (Thumb, 32 bytes, Stack size 12 bytes, stm32f10x_dac.o(.text), UNUSED)

  DAC_GetDataOutputValue (Thumb, 32 bytes, Stack size 8 bytes, stm32f10x_dac.o(.text), UNUSED)

  __use_no_semihosting (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi_2.o(.text), UNUSED)

  __2printf (Thumb, 20 bytes, Stack size 24 bytes, noretval__2printf.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = __2printf ⇒ _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _printf_char_file
  [Called By]
  - >> Soft_SPI_Read_Reg
  - >> bsp_init
  - >> PLL_Out_Ctr
  - >> PLL_Out_Amp
  - >> Key_Scan_Process
  - >> main
  - >> DDS_Out_Amp
  - >> Soft_SPI_WriteByte
  - >> _EC11_Freq_Step_Down
  - >> _EC11_Amp_Step_Down
  - >> _EC11_Freq_Step_Up
  - >> _EC11_Amp_Step_Up

  __2sprintf (Thumb, 34 bytes, Stack size 32 bytes, noretval__2sprintf.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> Freq_Value_to_ASCII_PLL
  - >> Freq_Value_to_ASCII
  - >> Amp_Value_to_ASCII
  - >> Power_menu_dBm_show

  _printf_pre_padding (Thumb, 44 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_int_common

  _printf_post_padding (Thumb, 34 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_int_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_u

  _printf_longlong_dec (Thumb, 108 bytes, Stack size 24 bytes, _printf_longlong_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  - >> _ll_udiv10
  [Called By]
  - >> _printf_llu

  __printf (Thumb, 388 bytes, Stack size 40 bytes, __printf_flags_ss_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  atoi (Thumb, 26 bytes, Stack size 16 bytes, atoi.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = atoi ⇒ strtol ⇒ _strtoul
  [Calls]
  - >> strtol
  - >> __aeabi_errno_addr
  [Called By]
  - >> Freq_ASC_to_Value

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> _fp_value
  - >> _strtoul
  - >> strtol
  - >> __set_errno
  - >> __read_errno
  - >> atoi

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  _ll_udiv10 (Thumb, 138 bytes, Stack size 12 bytes, lludiv10.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = _ll_udiv10
  [Called By]
  - >> _fp_digits
  - >> _printf_longlong_dec

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __read_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> atof

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> ldexp
  - >> __mathlib_tofloat
  - >> sqrt
  - >> pow
  - >> atof

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_longlong_dec
  - >> _printf_int_dec

  __lib_sel_fp_printf (Thumb, 2 bytes, Stack size 0 bytes, _printf_fp_dec.o(.text), UNUSED)

  _printf_fp_dec_real (Thumb, 620 bytes, Stack size 104 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 320
  - Call Chain = _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_infnan
  - >> __rt_locale
  - >> __ARM_fpclassify
  - >> _fp_digits
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> __2sprintf
  - >> _printf_char_file

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __2sprintf
  [Address Reference Count : 1]
  - noretval__2sprintf.o(.text)

  _printf_char_file (Thumb, 32 bytes, Stack size 16 bytes, _printf_char_file.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = _printf_char_file ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ferror
  - >> _printf_char_common
  [Called By]
  - >> __2printf

  __strtod_int (Thumb, 90 bytes, Stack size 40 bytes, strtod.o(.text))
  [Stack]

  - Max Depth = 424
  - Call Chain = __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _local_sscanf
  [Called By]
  - >> atof

  strtol (Thumb, 112 bytes, Stack size 32 bytes, strtol.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = strtol ⇒ _strtoul
  [Calls]
  - >> _strtoul
  - >> __rt_ctype_table
  - >> __aeabi_errno_addr
  [Called By]
  - >> atoi

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __rt_ctype_table (Thumb, 16 bytes, Stack size 8 bytes, rt_ctype_table.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __rt_ctype_table
  [Calls]
  - >> __rt_locale
  [Called By]
  - >> isspace
  - >> strtol

  __rt_locale (Thumb, 8 bytes, Stack size 0 bytes, rt_locale_intlibspace.o(.text))
  [Called By]

  - >> __rt_lib_init_lc_common
  - >> _scanf_really_real
  - >> __rt_ctype_table
  - >> _printf_fp_dec_real

  isspace (Thumb, 18 bytes, Stack size 8 bytes, isspace.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = isspace ⇒ __rt_ctype_table
  [Calls]
  - >> __rt_ctype_table
  [Address Reference Count : 1]
  - strtod.o(.text)

  _printf_fp_infnan (Thumb, 112 bytes, Stack size 24 bytes, _printf_fp_infnan.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_fp_infnan ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec_real

  _sgetc (Thumb, 30 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - strtod.o(.text)

  _sbackspace (Thumb, 34 bytes, Stack size 0 bytes, _sgetc.o(.text))
  [Address Reference Count : 1]

  - strtod.o(.text)

  _strtoul (Thumb, 158 bytes, Stack size 40 bytes, _strtoul.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _strtoul
  [Calls]
  - >> _chval
  - >> __aeabi_errno_addr
  [Called By]
  - >> strtol

  _btod_etento (Thumb, 216 bytes, Stack size 72 bytes, bigflt0.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  [Called By]
  - >> _fp_value
  - >> _fp_digits

  ferror (Thumb, 8 bytes, Stack size 0 bytes, ferror.o(.text))
  [Called By]

  - >> _printf_char_file

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  _chval (Thumb, 28 bytes, Stack size 0 bytes, _chval.o(.text))
  [Called By]

  - >> _scanf_really_hex_real
  - >> _strtoul

  _scanf_really_real (Thumb, 668 bytes, Stack size 120 bytes, scanf_fp.o(.text))
  [Stack]

  - Max Depth = 328
  - Call Chain = _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> __mathlib_narrow
  - >> _scanf_infnan
  - >> _scanf_hex_real
  - >> _fp_value
  - >> __rt_locale
  - >> _is_digit
  [Called By]
  - >> _scanf_real

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> _get_lc_ctype
  - >> _get_lc_numeric

  _scanf_really_hex_real (Thumb, 786 bytes, Stack size 80 bytes, scanf_hexfp.o(.text))
  [Stack]

  - Max Depth = 144
  - Call Chain = _scanf_really_hex_real ⇒ __support_ldexp ⇒ ldexp ⇒ __aeabi_cdcmpeq
  [Calls]
  - >> __support_ldexp
  - >> __aeabi_llsl
  - >> __mathlib_narrow
  - >> _chval
  [Called By]
  - >> _scanf_hex_real

  _scanf_really_infnan (Thumb, 292 bytes, Stack size 72 bytes, scanf_infnan.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _scanf_really_infnan
  [Called By]
  - >> _scanf_infnan

  __aeabi_llsl (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _scanf_really_hex_real

  _ll_shift_l (Thumb, 38 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  _btod_d2e (Thumb, 62 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e))
  [Calls]

  - >> _d2e_norm_op1
  [Called By]
  - >> _fp_digits

  _d2e_denorm_low (Thumb, 70 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_denorm_low))
  [Called By]

  - >> _d2e_norm_op1

  _d2e_norm_op1 (Thumb, 96 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_norm_op1))
  [Calls]

  - >> _d2e_denorm_low
  [Called By]
  - >> _btod_d2e

  __btod_div_common (Thumb, 696 bytes, Stack size 24 bytes, btod.o(CL$$btod_div_common))
  [Stack]

  - Max Depth = 24
  - Call Chain = __btod_div_common
  [Called By]
  - >> _btod_edivd
  - >> _btod_ediv

  _e2d (Thumb, 80 bytes, Stack size 8 bytes, btod.o(CL$$btod_e2d))
  [Stack]

  - Max Depth = 32
  - Call Chain = _e2d ⇒ _e2e
  [Calls]
  - >> _e2e
  [Called By]
  - >> _btod_emuld
  - >> _btod_edivd

  _e2e (Thumb, 198 bytes, Stack size 24 bytes, btod.o(CL$$btod_e2e))
  [Stack]

  - Max Depth = 24
  - Call Chain = _e2e
  [Called By]
  - >> _btod_emul
  - >> _btod_ediv
  - >> _e2d

  _btod_ediv (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_ediv))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_ediv ⇒ _e2e
  [Calls]
  - >> _e2e
  - >> __btod_div_common
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  _btod_edivd (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_edivd))
  [Stack]

  - Max Depth = 56
  - Call Chain = _btod_edivd ⇒ _e2d ⇒ _e2e
  [Calls]
  - >> _e2d
  - >> __btod_div_common
  [Called By]
  - >> _fp_value

  _btod_emul (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_emul))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_emul ⇒ _e2e
  [Calls]
  - >> __btod_mult_common
  - >> _e2e
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  _btod_emuld (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_emuld))
  [Stack]

  - Max Depth = 56
  - Call Chain = _btod_emuld ⇒ _e2d ⇒ _e2e
  [Calls]
  - >> __btod_mult_common
  - >> _e2d
  [Called By]
  - >> _fp_value

  __btod_mult_common (Thumb, 580 bytes, Stack size 16 bytes, btod.o(CL$$btod_mult_common))
  [Stack]

  - Max Depth = 16
  - Call Chain = __btod_mult_common
  [Called By]
  - >> _btod_emuld
  - >> _btod_emul

  __ARM_fpclassify (Thumb, 40 bytes, Stack size 0 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Called By]

  - >> _printf_fp_dec_real
  - >> pow

  __kernel_poly (Thumb, 170 bytes, Stack size 24 bytes, poly.o(i.__kernel_poly))
  [Stack]

  - Max Depth = 56
  - Call Chain = __kernel_poly ⇒ __aeabi_dmul
  [Calls]
  - >> __aeabi_dmul
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __mathlib_dbl_divzero (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_divzero))
  [Stack]

  - Max Depth = 32
  - Call Chain = __mathlib_dbl_divzero ⇒ __aeabi_ddiv
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_infnan2 (Thumb, 4 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_infnan2))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_infnan2 ⇒ __aeabi_dadd
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __mathlib_dbl_invalid (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_invalid))
  [Stack]

  - Max Depth = 32
  - Call Chain = __mathlib_dbl_invalid ⇒ __aeabi_ddiv
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_overflow (Thumb, 14 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_overflow))
  [Calls]

  - >> __ARM_scalbn
  [Called By]
  - >> ldexp
  - >> pow

  __mathlib_dbl_underflow (Thumb, 10 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_underflow))
  [Calls]

  - >> __ARM_scalbn
  [Called By]
  - >> ldexp
  - >> pow

  __mathlib_narrow (Thumb, 16 bytes, Stack size 8 bytes, narrow.o(i.__mathlib_narrow))
  [Stack]

  - Max Depth = 64
  - Call Chain = __mathlib_narrow ⇒ __mathlib_tofloat ⇒ __aeabi_cdcmpeq
  [Calls]
  - >> __mathlib_tofloat
  [Called By]
  - >> _scanf_really_hex_real
  - >> _scanf_really_real

  __mathlib_tofloat (Thumb, 132 bytes, Stack size 24 bytes, narrow.o(i.__mathlib_tofloat))
  [Stack]

  - Max Depth = 56
  - Call Chain = __mathlib_tofloat ⇒ __aeabi_cdcmpeq
  [Calls]
  - >> frexp
  - >> __aeabi_cdcmpeq
  - >> __set_errno
  - >> __aeabi_cdrcmple
  - >> __aeabi_d2f
  [Called By]
  - >> __mathlib_narrow

  __support_ldexp (Thumb, 22 bytes, Stack size 8 bytes, ldexp.o(i.__support_ldexp))
  [Stack]

  - Max Depth = 64
  - Call Chain = __support_ldexp ⇒ ldexp ⇒ __aeabi_cdcmpeq
  [Calls]
  - >> ldexp
  [Called By]
  - >> _scanf_really_hex_real

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> _scanf_really_real
  - >> __printf

  atof (Thumb, 42 bytes, Stack size 24 bytes, atof.o(i.atof))
  [Stack]

  - Max Depth = 448
  - Call Chain = atof ⇒ __strtod_int ⇒ _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> __strtod_int
  - >> __set_errno
  - >> __read_errno
  [Called By]
  - >> Amp_ASC_to_Value
  - >> Freq_ASC_to_Value_PLL

  frexp (Thumb, 80 bytes, Stack size 8 bytes, frexp.o(i.frexp))
  [Stack]

  - Max Depth = 8
  - Call Chain = frexp
  [Calls]
  - >> __ARM_scalbn
  [Called By]
  - >> __mathlib_tofloat

  ldexp (Thumb, 116 bytes, Stack size 24 bytes, ldexp.o(i.ldexp))
  [Stack]

  - Max Depth = 56
  - Call Chain = ldexp ⇒ __aeabi_cdcmpeq
  [Calls]
  - >> __aeabi_cdcmpeq
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __ARM_scalbn
  - >> __set_errno
  [Called By]
  - >> __support_ldexp

  pow (Thumb, 2512 bytes, Stack size 128 bytes, pow.o(i.pow))
  [Stack]

  - Max Depth = 192
  - Call Chain = pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __kernel_poly
  - >> __ARM_fpclassify
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_infnan2
  - >> __mathlib_dbl_divzero
  - >> __ARM_scalbn
  - >> __set_errno
  - >> sqrt
  - >> __aeabi_cdrcmple
  - >> __aeabi_dmul
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dadd
  [Called By]
  - >> Get_Adc_Rms

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> Get_Adc_Rms
  - >> pow

  _get_lc_numeric (Thumb, 44 bytes, Stack size 8 bytes, lc_numeric_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_numeric
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_numeric_2

  _get_lc_ctype (Thumb, 44 bytes, Stack size 8 bytes, lc_ctype_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_ctype
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_ctype_2
  [Address Reference Count : 1]
  - rt_ctype_table.o(.text)

  __aeabi_d2f (Thumb, 0 bytes, Stack size 32 bytes, d2f.o(x$fpl$d2f))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2f
  [Called By]
  - >> Amp_ASC_to_Value
  - >> __mathlib_tofloat

  _d2f (Thumb, 98 bytes, Stack size 32 bytes, d2f.o(x$fpl$d2f), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_dnaninf

  __aeabi_dadd (Thumb, 0 bytes, Stack size 16 bytes, daddsub_clz.o(x$fpl$dadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_dadd
  [Called By]
  - >> Get_Adc_LPF
  - >> Get_Adc_Rms
  - >> DDS_Out_Amp
  - >> __kernel_poly
  - >> __mathlib_dbl_infnan2
  - >> pow

  _dadd (Thumb, 332 bytes, Stack size 16 bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf
  - >> _dsub1

  __fpl_dcheck_NaN1 (Thumb, 10 bytes, Stack size 0 bytes, dcheck1.o(x$fpl$dcheck1))
  [Calls]

  - >> __fpl_return_NaN
  [Called By]
  - >> __ARM_scalbn

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmpeq
  - >> _dcmple

  __aeabi_ddiv (Thumb, 0 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_ddiv
  [Called By]
  - >> Get_Adc_Rms
  - >> CH2_Freq_Set
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_divzero
  - >> pow

  _ddiv (Thumb, 552 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __aeabi_cdcmpeq (Thumb, 0 bytes, Stack size 32 bytes, deqf.o(x$fpl$deqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmpeq
  [Called By]
  - >> ldexp
  - >> __mathlib_tofloat

  _dcmpeq (Thumb, 120 bytes, Stack size 32 bytes, deqf.o(x$fpl$deqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __aeabi_d2uiz (Thumb, 0 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2uiz
  [Called By]
  - >> Get_Adc_LPF
  - >> Get_Adc_Rms
  - >> AD9912_Phase_Convert
  - >> Set_LMX2592_Freq_RealTime
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO

  _dfixu (Thumb, 90 bytes, Stack size 32 bytes, dfixu.o(x$fpl$dfixu), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt))
  [Called By]

  - >> pow

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_ui2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu))
  [Called By]

  - >> Get_Adc_LPF
  - >> Get_Adc_Rms
  - >> DDS_Out_Amp
  - >> AD9912_Phase_Convert
  - >> AD9912_Freq_Convert_Hz
  - >> AD9912_Freq_Convert
  - >> Set_LMX2592_Freq_RealTime
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO

  _dfltu (Thumb, 38 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dfltu), UNUSED)

  __aeabi_ul2d (Thumb, 0 bytes, Stack size 8 bytes, dfltll_clz.o(x$fpl$dfltull))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_ul2d
  [Called By]
  - >> CH2_Freq_Set

  _ll_uto_d (Thumb, 138 bytes, Stack size 8 bytes, dfltll_clz.o(x$fpl$dfltull), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_cdcmple
  [Called By]
  - >> CH2_Freq_Set
  - >> DDS_Out_Amp
  - >> Set_LMX2592_Freq_RealTime

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> __fpl_dcmp_Inf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __aeabi_dmul (Thumb, 0 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dmul
  [Called By]
  - >> Get_Adc_LPF
  - >> AD9912_Phase_Convert
  - >> AD9912_Freq_Convert_Hz
  - >> AD9912_Freq_Convert
  - >> Set_LMX2592_Freq_RealTime
  - >> LMX2592_OUT_DIV
  - >> LMX2592_OUT_VCO
  - >> __kernel_poly
  - >> pow

  _dmul (Thumb, 332 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _dcmpeq
  - >> _dsqrt
  - >> _dmul
  - >> _dcmple
  - >> _ll_ufrom_d
  - >> _dfixu
  - >> _ddiv
  - >> _dsub
  - >> _dadd
  - >> _d2f

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _f2d
  - >> _dmul
  - >> _ddiv
  - >> _dadd

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> CH2_Freq_Set
  - >> DDS_Out_Amp
  - >> Set_LMX2592_Freq_RealTime
  - >> __mathlib_tofloat
  - >> pow

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  __aeabi_drsub (Thumb, 0 bytes, Stack size 8 bytes, daddsub_clz.o(x$fpl$drsb))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_drsub
  [Called By]
  - >> pow

  _drsb (Thumb, 22 bytes, Stack size 8 bytes, daddsub_clz.o(x$fpl$drsb), UNUSED)
  [Calls]

  - >> _dsub1
  - >> _dadd1

  _dsqrt (Thumb, 456 bytes, Stack size 24 bytes, dsqrt_noumaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> sqrt

  __aeabi_dsub (Thumb, 0 bytes, Stack size 32 bytes, daddsub_clz.o(x$fpl$dsub))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dsub
  [Called By]
  - >> Get_Adc_LPF
  - >> pow

  _dsub (Thumb, 464 bytes, Stack size 32 bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)
  [Calls]

  - >> __fpl_dnaninf
  - >> _dadd1

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> Amp_Value_to_ASCII
  - >> main
  - >> DDS_Out_Amp
  - >> Power_menu_dBm_show

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __aeabi_fadd (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fadd
  [Called By]
  - >> PLL_Out_Amp
  - >> DDS_Out_Amp
  - >> _EC11_Amp_Step_Up
  - >> ADL5513_dBm_Out

  _fadd (Thumb, 196 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf
  - >> _fsub1

  __fpl_fcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, fcmpi.o(x$fpl$fcmpinf), UNUSED)
  [Called By]

  - >> _fcmple
  - >> _fcmpeq

  __aeabi_fdiv (Thumb, 0 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fdiv
  [Called By]
  - >> Dac1_Set_Vol
  - >> ADL5513_dBm_Out

  _fdiv (Thumb, 384 bytes, Stack size 16 bytes, fdiv.o(x$fpl$fdiv), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __aeabi_cfcmpeq (Thumb, 0 bytes, Stack size 16 bytes, feqf.o(x$fpl$feqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cfcmpeq
  [Called By]
  - >> Oled_Main_Task
  - >> main

  _fcmpeq (Thumb, 104 bytes, Stack size 16 bytes, feqf.o(x$fpl$feqf), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_fcmp_Inf

  __aeabi_f2uiz (Thumb, 0 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2uiz
  [Called By]
  - >> Dac1_Set_Vol
  - >> PLL_Out_Amp
  - >> DDS_Out_Amp

  _ffixu (Thumb, 62 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_ui2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu))
  [Called By]

  - >> Dac1_Set_Vol
  - >> ADL5513_dBm_Out

  _ffltu (Thumb, 38 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu), UNUSED)

  __aeabi_cfcmple (Thumb, 0 bytes, Stack size 16 bytes, fleqf.o(x$fpl$fleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cfcmple
  [Called By]
  - >> PLL_Out_Amp
  - >> main
  - >> DDS_Out_Amp
  - >> _EC11_Amp_Step_Down
  - >> _EC11_Amp_Step_Up
  - >> ADL5513_dBm_Out
  - >> Power_menu_dBm_show

  _fcmple (Thumb, 104 bytes, Stack size 16 bytes, fleqf.o(x$fpl$fleqf), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_fcmp_Inf

  __fpl_fcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, fleqf.o(x$fpl$fleqf), UNUSED)
  [Called By]

  - >> _frcmple

  __aeabi_fmul (Thumb, 0 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> Dac1_Set_Vol
  - >> ADL5513_dBm_Out

  _fmul (Thumb, 258 bytes, Stack size 16 bytes, fmul.o(x$fpl$fmul), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_fnaninf

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _fcmple
  - >> _ffixu
  - >> _fcmpeq
  - >> _fdiv
  - >> _fsub
  - >> _fadd
  - >> _f2d

  __fpl_fretinf (Thumb, 10 bytes, Stack size 0 bytes, fretinf.o(x$fpl$fretinf), UNUSED)
  [Called By]

  - >> _fmul
  - >> _fdiv
  - >> _fadd
  - >> _d2f

  __aeabi_cfrcmple (Thumb, 0 bytes, Stack size 0 bytes, frleqf.o(x$fpl$frleqf))
  [Called By]

  - >> PLL_Out_Amp
  - >> main
  - >> DDS_Out_Amp
  - >> _EC11_Amp_Step_Down
  - >> _EC11_Amp_Step_Up
  - >> ADL5513_dBm_Out
  - >> Power_menu_dBm_show

  _frcmple (Thumb, 98 bytes, Stack size 0 bytes, frleqf.o(x$fpl$frleqf), UNUSED)
  [Calls]

  - >> __fpl_fcmple_InfNaN

  __aeabi_frsub (Thumb, 0 bytes, Stack size 0 bytes, faddsub_clz.o(x$fpl$frsb))
  [Called By]

  - >> PLL_Out_Amp
  - >> DDS_Out_Amp

  _frsb (Thumb, 20 bytes, Stack size 0 bytes, faddsub_clz.o(x$fpl$frsb), UNUSED)
  [Calls]

  - >> _fsub1
  - >> _fadd1

  __aeabi_fsub (Thumb, 0 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_fsub
  [Called By]
  - >> DDS_Out_Amp
  - >> _EC11_Amp_Step_Down
  - >> ADL5513_dBm_Out

  _fsub (Thumb, 234 bytes, Stack size 16 bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> _fadd1

  __aeabi_d2ulz (Thumb, 0 bytes, Stack size 32 bytes, dfixull.o(x$fpl$llufromd))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2ulz
  [Called By]
  - >> AD9912_Freq_Convert_Hz
  - >> AD9912_Freq_Convert
  - >> Freq_ASC_to_Value_PLL

  _ll_ufrom_d (Thumb, 120 bytes, Stack size 32 bytes, dfixull.o(x$fpl$llufromd), UNUSED)
  [Calls]

  - >> __fpl_dnaninf

  _printf_fp_dec (Thumb, 4 bytes, Stack size 0 bytes, printf1.o(x$fpl$printf1))
  [Stack]

  - Max Depth = 320
  - Call Chain = _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec_real
  [Called By]
  - >> _printf_f

  __fpl_return_NaN (Thumb, 100 bytes, Stack size 0 bytes, retnan.o(x$fpl$retnan))
  [Calls]

  - >> __fpl_cmpreturn
  [Called By]
  - >> __fpl_dcheck_NaN1

  __ARM_scalbn (Thumb, 92 bytes, Stack size 0 bytes, scalbn.o(x$fpl$scalbn))
  [Calls]

  - >> __fpl_dcheck_NaN1
  [Called By]
  - >> ldexp
  - >> frexp
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> pow

  _scanf_real (Thumb, 4 bytes, Stack size 0 bytes, scanf1.o(x$fpl$scanf1))
  [Stack]

  - Max Depth = 328
  - Call Chain = _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _scanf_really_real
  [Called By]
  - >> _local_sscanf

  _scanf_hex_real (Thumb, 4 bytes, Stack size 0 bytes, scanf2.o(x$fpl$scanf2))
  [Stack]

  - Max Depth = 144
  - Call Chain = _scanf_hex_real ⇒ _scanf_really_hex_real ⇒ __support_ldexp ⇒ ldexp ⇒ __aeabi_cdcmpeq
  [Calls]
  - >> _scanf_really_hex_real
  [Called By]
  - >> _scanf_really_real

  _scanf_infnan (Thumb, 4 bytes, Stack size 0 bytes, scanf2.o(x$fpl$scanf2))
  [Stack]

  - Max Depth = 72
  - Call Chain = _scanf_infnan ⇒ _scanf_really_infnan
  [Calls]
  - >> _scanf_really_infnan
  [Called By]
  - >> _scanf_really_real

  __fpl_cmpreturn (Thumb, 48 bytes, Stack size 0 bytes, trapv.o(x$fpl$trapveneer))
  [Called By]

  - >> __fpl_return_NaN

  ### Local Symbols

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  IsKeyDownS1 (Thumb, 18 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Address Reference Count : 1]

  - matrix_key.o(.text)

  IsKeyDownS2 (Thumb, 18 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Address Reference Count : 1]

  - matrix_key.o(.text)

  IsKeyDownS3 (Thumb, 18 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Address Reference Count : 1]

  - matrix_key.o(.text)

  IsKeyDownS4 (Thumb, 18 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Address Reference Count : 1]

  - matrix_key.o(.text)

  IsKeyDownENT (Thumb, 18 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Address Reference Count : 1]

  - matrix_key.o(.text)

  bsp_InitKeyVar (Thumb, 110 bytes, Stack size 0 bytes, matrix_key.o(.text))
  [Called By]

  - >> bsp_InitKey

  bsp_InitKeyHard (Thumb, 136 bytes, Stack size 8 bytes, matrix_key.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = bsp_InitKeyHard ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> bsp_InitKey

  bsp_DetectKey (Thumb, 198 bytes, Stack size 16 bytes, matrix_key.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = bsp_DetectKey
  [Calls]
  - >> bsp_PutKey
  [Called By]
  - >> bsp_KeyScan

  TI4_Config (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TI4_Config
  [Called By]
  - >> TIM_ICInit

  TI3_Config (Thumb, 122 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TI3_Config
  [Called By]
  - >> TIM_ICInit

  TI2_Config (Thumb, 130 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TI2_Config
  [Called By]
  - >> TIM_ICInit
  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig

  TI1_Config (Thumb, 108 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TI1_Config
  [Called By]
  - >> TIM_ICInit
  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig

  _dadd1 (Thumb, 0 bytes, Stack size unknown bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)
  [Called By]

  - >> _dsub
  - >> _drsb

  _dsub1 (Thumb, 0 bytes, Stack size unknown bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)
  [Called By]

  - >> _drsb
  - >> _dadd

  _fadd1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fadd), UNUSED)
  [Called By]

  - >> _fsub
  - >> _frsb

  _fsub1 (Thumb, 0 bytes, Stack size unknown bytes, faddsub_clz.o(x$fpl$fsub), UNUSED)
  [Called By]

  - >> _frsb
  - >> _fadd

  _fp_digits (Thumb, 428 bytes, Stack size 96 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  - >> _btod_d2e
  - >> _btod_etento
  - >> _ll_udiv10
  [Called By]
  - >> _printf_fp_dec_real

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  _local_sscanf (Thumb, 60 bytes, Stack size 56 bytes, strtod.o(.text))
  [Stack]

  - Max Depth = 384
  - Call Chain = _local_sscanf ⇒ _scanf_real ⇒ _scanf_really_real ⇒ _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _scanf_real
  [Called By]
  - >> __strtod_int

  _fp_value (Thumb, 508 bytes, Stack size 88 bytes, scanf_fp.o(.text))
  [Stack]

  - Max Depth = 208
  - Call Chain = _fp_value ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emuld
  - >> _btod_edivd
  - >> _btod_etento
  - >> __aeabi_errno_addr
  [Called By]
  - >> _scanf_really_real

  ### Undefined Global Symbols