Static Call Graph - [STM32F030C8\QQ527148813.axf]

# Static Call Graph for image STM32F030C8\QQ527148813.axf

#<CALLGRAPH># ARM Linker, 5060528: Last Updated: Sun Jul 19 14:39:13 2020

### Maximum Stack Usage = 172 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod

### Mutually Recursive functions

- ADC1_IRQHandler ⇒ ADC1_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- _Error_Handler ⇒ _Error_Handler

  ### Function Pointers

  - ADC1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - ADC_DMAConvCplt from stm32f0xx_hal_adc.o(i.ADC_DMAConvCplt) referenced from stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA)
  - ADC_DMAError from stm32f0xx_hal_adc.o(i.ADC_DMAError) referenced from stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA)
  - ADC_DMAHalfConvCplt from stm32f0xx_hal_adc.o(i.ADC_DMAHalfConvCplt) referenced from stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA)
  - DMA1_Channel1_IRQHandler from stm32f0xx_it.o(i.DMA1_Channel1_IRQHandler) referenced from startup_stm32f030x8.o(RESET)
  - DMA1_Channel2_3_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - DMA1_Channel4_5_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - EXTI0_1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - EXTI2_3_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - EXTI4_15_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - FLASH_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - HardFault_Handler from stm32f0xx_it.o(i.HardFault_Handler) referenced from startup_stm32f030x8.o(RESET)
  - I2C1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - I2C2_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - NMI_Handler from stm32f0xx_it.o(i.NMI_Handler) referenced from startup_stm32f030x8.o(RESET)
  - PendSV_Handler from stm32f0xx_it.o(i.PendSV_Handler) referenced from startup_stm32f030x8.o(RESET)
  - RCC_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - RTC_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - Reset_Handler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SPI1_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SPI2_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - SVC_Handler from stm32f0xx_it.o(i.SVC_Handler) referenced from startup_stm32f030x8.o(RESET)
  - SysTick_Handler from stm32f0xx_it.o(i.SysTick_Handler) referenced from startup_stm32f030x8.o(RESET)
  - SystemInit from system_stm32f0xx.o(i.SystemInit) referenced from startup_stm32f030x8.o(.text)
  - TIM14_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM15_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM16_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM17_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM1_BRK_UP_TRG_COM_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - TIM3_IRQHandler from stm32f0xx_it.o(i.TIM3_IRQHandler) referenced from startup_stm32f030x8.o(RESET)
  - TIM6_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - UART_DMAAbortOnError from stm32f0xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f0xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - USART1_IRQHandler from stm32f0xx_it.o(i.USART1_IRQHandler) referenced from startup_stm32f030x8.o(RESET)
  - USART2_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - WWDG_IRQHandler from startup_stm32f030x8.o(.text) referenced from startup_stm32f030x8.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f030x8.o(.text)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Calls]

  - >> ADC1_IRQHandler
  [Called By]
  - >> ADC1_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  DMA1_Channel2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  DMA1_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  EXTI0_1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  EXTI2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  EXTI4_15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM1_BRK_UP_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f030x8.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_uidivmod
  [Called By]
  - >> HAL_InitTick
  - >> HAL_RCC_GetSysClockFreq
  - >> UART_SetConfig
  - >> HAL_ADC_ConfigChannel
  - >> SystemClock_Config
  - >> DMA_CalcBaseAndBitshift
  - >> LED_DataHandle
  - >> ADC_Enable

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  DMA1_Channel1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.DMA1_Channel1_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA1_Channel1_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  FLASH_Init (Thumb, 22 bytes, Stack size 4 bytes, flash.o(i.FLASH_Init))
  [Stack]

  - Max Depth = 4
  - Call Chain = FLASH_Init
  [Calls]
  - >> FLASH_Read
  [Called By]
  - >> USER_Init

  FLASH_Read (Thumb, 56 bytes, Stack size 0 bytes, flash.o(i.FLASH_Read))
  [Called By]

  - >> FLASH_Init

  HAL_ADCEx_Calibration_Start (Thumb, 176 bytes, Stack size 24 bytes, stm32f0xx_hal_adc_ex.o(i.HAL_ADCEx_Calibration_Start))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_ADCEx_Calibration_Start
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> myADC_Start

  HAL_ADC_ConfigChannel (Thumb, 254 bytes, Stack size 24 bytes, stm32f0xx_hal_adc.o(i.HAL_ADC_ConfigChannel))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_ADC_ConfigChannel ⇒ __aeabi_uidivmod
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> MX_ADC_Init

  HAL_ADC_ConvCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_adc.o(i.HAL_ADC_ConvCpltCallback))
  [Called By]

  - >> ADC_DMAConvCplt

  HAL_ADC_ConvHalfCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_adc.o(i.HAL_ADC_ConvHalfCpltCallback))
  [Called By]

  - >> ADC_DMAHalfConvCplt

  HAL_ADC_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_adc.o(i.HAL_ADC_ErrorCallback))
  [Called By]

  - >> ADC_DMAError

  HAL_ADC_Init (Thumb, 364 bytes, Stack size 24 bytes, stm32f0xx_hal_adc.o(i.HAL_ADC_Init))
  [Stack]

  - Max Depth = 108
  - Call Chain = HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_ADC_MspInit
  [Called By]
  - >> MX_ADC_Init
  - >> myADC_Start

  HAL_ADC_MspInit (Thumb, 104 bytes, Stack size 48 bytes, adc.o(i.HAL_ADC_MspInit))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_ADC_MspInit ⇒ HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_DMA_Init
  - >> _Error_Handler
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_ADC_Init

  HAL_ADC_Start_DMA (Thumb, 144 bytes, Stack size 32 bytes, stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_ADC_Start_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  - >> ADC_Enable
  [Called By]
  - >> myADC_Start

  HAL_DMA_Abort_IT (Thumb, 72 bytes, Stack size 16 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_IRQHandler (Thumb, 156 bytes, Stack size 16 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_DMA_IRQHandler
  [Called By]
  - >> DMA1_Channel1_IRQHandler

  HAL_DMA_Init (Thumb, 84 bytes, Stack size 16 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> DMA_CalcBaseAndBitshift
  [Called By]
  - >> HAL_ADC_MspInit

  HAL_DMA_Start_IT (Thumb, 106 bytes, Stack size 24 bytes, stm32f0xx_hal_dma.o(i.HAL_DMA_Start_IT))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> DMA_SetConfig
  [Called By]
  - >> HAL_ADC_Start_DMA

  HAL_GPIO_Init (Thumb, 302 bytes, Stack size 24 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_ADC_MspInit
  - >> MX_GPIO_Init
  - >> HAL_UART_MspInit

  HAL_GPIO_WritePin (Thumb, 12 bytes, Stack size 0 bytes, stm32f0xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> MX_GPIO_Init
  - >> LED_SetData
  - >> LED_SetDIGx
  - >> LED_DataHandle

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_IWDG_Init
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_ADCEx_Calibration_Start
  - >> ADC_Enable

  HAL_IWDG_Init (Thumb, 86 bytes, Stack size 16 bytes, stm32f0xx_hal_iwdg.o(i.HAL_IWDG_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_IWDG_Init
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> MX_IWDG_Init

  HAL_IWDG_Refresh (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_hal_iwdg.o(i.HAL_IWDG_Refresh))
  [Called By]

  - >> main

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f0xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_InitTick
  - >> HAL_MspInit
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f0xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_InitTick ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_NVIC_SetPriority
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 50 bytes, Stack size 8 bytes, stm32f0xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 14 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_TIM_Base_MspInit
  - >> MX_DMA_Init
  - >> main

  HAL_NVIC_SetPriority (Thumb, 8 bytes, Stack size 8 bytes, stm32f0xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> HAL_MspInit
  - >> HAL_TIM_Base_MspInit
  - >> MX_DMA_Init
  - >> main
  - >> SystemClock_Config

  HAL_RCCEx_PeriphCLKConfig (Thumb, 218 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 280 bytes, Stack size 24 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 6 bytes, Stack size 0 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Called By]

  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 76 bytes, Stack size 40 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 52
  - Call Chain = HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> UART_SetConfig
  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 840 bytes, Stack size 32 bytes, stm32f0xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 38 bytes, Stack size 8 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick
  - >> SystemClock_Config

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f0xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_BreakCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim_ex.o(i.HAL_TIMEx_BreakCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_CommutationCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim_ex.o(i.HAL_TIMEx_CommutationCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 72 bytes, Stack size 16 bytes, stm32f0xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init

  HAL_TIM_Base_Init (Thumb, 52 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init

  HAL_TIM_Base_MspInit (Thumb, 66 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIM_Base_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start_IT (Thumb, 22 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_Base_Start_IT))
  [Called By]

  - >> TIME_Init

  HAL_TIM_ConfigClockSource (Thumb, 238 bytes, Stack size 24 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init

  HAL_TIM_IC_CaptureCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_IC_CaptureCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_IRQHandler (Thumb, 354 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ LED_DataHandle ⇒ LED_SetDIGx ⇒ __ARM_common_switch8
  [Calls]
  - >> HAL_TIMEx_CommutationCallback
  - >> HAL_TIMEx_BreakCallback
  - >> HAL_TIM_PeriodElapsedCallback
  - >> HAL_TIM_TriggerCallback
  - >> HAL_TIM_PWM_PulseFinishedCallback
  - >> HAL_TIM_OC_DelayElapsedCallback
  - >> HAL_TIM_IC_CaptureCallback
  [Called By]
  - >> TIM3_IRQHandler

  HAL_TIM_OC_DelayElapsedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_OC_DelayElapsedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PWM_PulseFinishedCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_PWM_PulseFinishedCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_TIM_PeriodElapsedCallback (Thumb, 38 bytes, Stack size 8 bytes, time.o(i.HAL_TIM_PeriodElapsedCallback))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIM_PeriodElapsedCallback ⇒ LED_DataHandle ⇒ LED_SetDIGx ⇒ __ARM_common_switch8
  [Calls]
  - >> LED_DataHandle
  [Called By]
  - >> HAL_TIM_IRQHandler

  HAL_TIM_SlaveConfigSynchronization (Thumb, 60 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_SlaveConfigSynchronization))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_TIM_SlaveConfigSynchronization ⇒ TIM_SlaveTimer_SetConfig ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_SlaveTimer_SetConfig
  [Called By]
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init

  HAL_TIM_TriggerCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.HAL_TIM_TriggerCallback))
  [Called By]

  - >> HAL_TIM_IRQHandler

  HAL_UART_ErrorCallback (Thumb, 12 bytes, Stack size 8 bytes, myuart.o(i.HAL_UART_ErrorCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UART_ErrorCallback
  [Calls]
  - >> _Error_Handler
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 272 bytes, Stack size 24 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_IRQHandler ⇒ UART_Receive_IT ⇒ HAL_UART_RxCpltCallback ⇒ HAL_UART_Receive_IT
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_UART_ErrorCallback
  - >> UART_Transmit_IT
  - >> UART_Receive_IT
  - >> UART_EndTransmit_IT
  - >> UART_EndRxTransfer
  [Called By]
  - >> USART1_IRQHandler

  HAL_UART_Init (Thumb, 108 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 92
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> UART_SetConfig
  - >> UART_CheckIdleState
  - >> UART_AdvFeatureConfig
  - >> HAL_UART_MspInit
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_UART_MspInit (Thumb, 64 bytes, Stack size 32 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  HAL_UART_Receive_IT (Thumb, 132 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.HAL_UART_Receive_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_UART_Receive_IT
  [Called By]
  - >> HAL_UART_RxCpltCallback
  - >> UART_Init

  HAL_UART_RxCpltCallback (Thumb, 90 bytes, Stack size 16 bytes, myuart.o(i.HAL_UART_RxCpltCallback))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_UART_RxCpltCallback ⇒ HAL_UART_Receive_IT
  [Calls]
  - >> HAL_UART_Receive_IT
  [Called By]
  - >> UART_Receive_IT

  HAL_UART_TxCpltCallback (Thumb, 22 bytes, Stack size 0 bytes, myuart.o(i.HAL_UART_TxCpltCallback))
  [Called By]

  - >> UART_EndTransmit_IT

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  KEY_Init (Thumb, 10 bytes, Stack size 0 bytes, key.o(i.KEY_Init))
  [Called By]

  - >> USER_Init

  LED_DataHandle (Thumb, 198 bytes, Stack size 24 bytes, led.o(i.LED_DataHandle))
  [Stack]

  - Max Depth = 56
  - Call Chain = LED_DataHandle ⇒ LED_SetDIGx ⇒ __ARM_common_switch8
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> __aeabi_uidivmod
  - >> LED_SetData
  - >> LED_SetDIGx
  [Called By]
  - >> HAL_TIM_PeriodElapsedCallback

  LED_Init (Thumb, 24 bytes, Stack size 0 bytes, led.o(i.LED_Init))
  [Called By]

  - >> USER_Init

  LED_SetDIGx (Thumb, 750 bytes, Stack size 24 bytes, led.o(i.LED_SetDIGx))
  [Stack]

  - Max Depth = 32
  - Call Chain = LED_SetDIGx ⇒ __ARM_common_switch8
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> __ARM_common_switch8
  [Called By]
  - >> LED_DataHandle

  LED_SetData (Thumb, 598 bytes, Stack size 16 bytes, led.o(i.LED_SetData))
  [Stack]

  - Max Depth = 24
  - Call Chain = LED_SetData ⇒ __ARM_common_switch8
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> __ARM_common_switch8
  [Called By]
  - >> LED_DataHandle

  MX_ADC_Init (Thumb, 94 bytes, Stack size 24 bytes, adc.o(i.MX_ADC_Init))
  [Stack]

  - Max Depth = 132
  - Call Chain = MX_ADC_Init ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_ADC_Init
  - >> HAL_ADC_ConfigChannel
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_DMA_Init (Thumb, 36 bytes, Stack size 8 bytes, dma.o(i.MX_DMA_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = MX_DMA_Init ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 192 bytes, Stack size 48 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_IWDG_Init (Thumb, 36 bytes, Stack size 8 bytes, iwdg.o(i.MX_IWDG_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = MX_IWDG_Init ⇒ HAL_IWDG_Init
  [Calls]
  - >> HAL_IWDG_Init
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_TIM1_Init (Thumb, 126 bytes, Stack size 56 bytes, tim.o(i.MX_TIM1_Init))
  [Stack]

  - Max Depth = 100
  - Call Chain = MX_TIM1_Init ⇒ HAL_TIM_SlaveConfigSynchronization ⇒ TIM_SlaveTimer_SetConfig ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> HAL_TIM_SlaveConfigSynchronization
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_TIM3_Init (Thumb, 124 bytes, Stack size 56 bytes, tim.o(i.MX_TIM3_Init))
  [Stack]

  - Max Depth = 100
  - Call Chain = MX_TIM3_Init ⇒ HAL_TIM_SlaveConfigSynchronization ⇒ TIM_SlaveTimer_SetConfig ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> HAL_TIM_SlaveConfigSynchronization
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> _Error_Handler
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 52 bytes, Stack size 8 bytes, usart.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 100
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> _Error_Handler
  - >> HAL_UART_Init
  [Called By]
  - >> main

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f0xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(RESET)

  SysTick_Handler (Thumb, 12 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  SystemClock_Config (Thumb, 124 bytes, Stack size 96 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 172
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_NVIC_SetPriority
  - >> __aeabi_uidivmod
  [Called By]
  - >> main

  SystemInit (Thumb, 78 bytes, Stack size 0 bytes, system_stm32f0xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f030x8.o(.text)

  TIM3_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.TIM3_IRQHandler))
  [Stack]

  - Max Depth = 88
  - Call Chain = TIM3_IRQHandler ⇒ HAL_TIM_IRQHandler ⇒ HAL_TIM_PeriodElapsedCallback ⇒ LED_DataHandle ⇒ LED_SetDIGx ⇒ __ARM_common_switch8
  [Calls]
  - >> HAL_TIM_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  TIME_Init (Thumb, 30 bytes, Stack size 8 bytes, time.o(i.TIME_Init))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIME_Init
  [Calls]
  - >> HAL_TIM_Base_Start_IT
  [Called By]
  - >> USER_Init

  TIM_Base_SetConfig (Thumb, 112 bytes, Stack size 20 bytes, stm32f0xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  TIM_ETR_SetConfig (Thumb, 22 bytes, Stack size 12 bytes, stm32f0xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource
  - >> TIM_SlaveTimer_SetConfig

  UART_AdvFeatureConfig (Thumb, 202 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_AdvFeatureConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_AdvFeatureConfig
  [Called By]
  - >> HAL_UART_Init

  UART_CheckIdleState (Thumb, 18 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_CheckIdleState))
  [Called By]

  - >> HAL_UART_Init

  UART_EndTransmit_IT (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_EndTransmit_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_EndTransmit_IT
  [Calls]
  - >> HAL_UART_TxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_Init (Thumb, 72 bytes, Stack size 8 bytes, myuart.o(i.UART_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_Init ⇒ HAL_UART_Receive_IT
  [Calls]
  - >> HAL_UART_Receive_IT
  [Called By]
  - >> USER_Init

  UART_Receive_IT (Thumb, 122 bytes, Stack size 16 bytes, stm32f0xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 48
  - Call Chain = UART_Receive_IT ⇒ HAL_UART_RxCpltCallback ⇒ HAL_UART_Receive_IT
  [Calls]
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 280 bytes, Stack size 24 bytes, stm32f0xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 76
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_RCC_GetPCLK1Freq
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_UART_Init

  UART_Transmit_IT (Thumb, 102 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_Transmit_IT))
  [Called By]

  - >> HAL_UART_IRQHandler

  USART1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_it.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 80
  - Call Chain = USART1_IRQHandler ⇒ HAL_UART_IRQHandler ⇒ UART_Receive_IT ⇒ HAL_UART_RxCpltCallback ⇒ HAL_UART_Receive_IT
  [Calls]
  - >> HAL_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f030x8.o(RESET)

  USER_Init (Thumb, 28 bytes, Stack size 8 bytes, user.o(i.USER_Init))
  [Stack]

  - Max Depth = 132
  - Call Chain = USER_Init ⇒ myADC_Init ⇒ myADC_Start ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> myADC_Init
  - >> UART_Init
  - >> TIME_Init
  - >> LED_Init
  - >> KEY_Init
  - >> FLASH_Init
  [Called By]
  - >> main

  USER_Run (Thumb, 70 bytes, Stack size 8 bytes, user.o(i.USER_Run))
  [Stack]

  - Max Depth = 20
  - Call Chain = USER_Run ⇒ myPC_handle
  [Calls]
  - >> myUSART_OverTime
  - >> myPC_handle
  [Called By]
  - >> main

  _Error_Handler (Thumb, 2 bytes, Stack size 0 bytes, main.o(i._Error_Handler))
  [Calls]

  - >> _Error_Handler
  [Called By]
  - >> HAL_ADC_MspInit
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init
  - >> MX_IWDG_Init
  - >> MX_ADC_Init
  - >> _Error_Handler
  - >> MX_USART1_UART_Init
  - >> myADC_Start
  - >> HAL_UART_ErrorCallback

  __ARM_common_switch8 (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal_dma.o(i.__ARM_common_switch8))
  [Stack]

  - Max Depth = 8
  - Call Chain = __ARM_common_switch8
  [Called By]
  - >> TIM_SlaveTimer_SetConfig
  - >> LED_SetData
  - >> LED_SetDIGx

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  main (Thumb, 72 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 172
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_RCC_GetSysClockFreq ⇒ __aeabi_uidivmod
  [Calls]
  - >> USER_Run
  - >> USER_Init
  - >> MX_TIM3_Init
  - >> MX_TIM1_Init
  - >> MX_IWDG_Init
  - >> MX_GPIO_Init
  - >> MX_DMA_Init
  - >> MX_ADC_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_Init
  - >> HAL_IWDG_Refresh
  - >> SystemClock_Config
  - >> MX_USART1_UART_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  myADC_Init (Thumb, 8 bytes, Stack size 8 bytes, myadc.o(i.myADC_Init))
  [Stack]

  - Max Depth = 124
  - Call Chain = myADC_Init ⇒ myADC_Start ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> myADC_Start
  [Called By]
  - >> USER_Init

  myADC_Start (Thumb, 50 bytes, Stack size 8 bytes, myadc.o(i.myADC_Start))
  [Stack]

  - Max Depth = 116
  - Call Chain = myADC_Start ⇒ HAL_ADC_Init ⇒ HAL_ADC_MspInit ⇒ HAL_DMA_Init ⇒ DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_ADC_Init
  - >> _Error_Handler
  - >> HAL_ADCEx_Calibration_Start
  - >> HAL_ADC_Start_DMA
  [Called By]
  - >> myADC_Init

  myPC_handle (Thumb, 60 bytes, Stack size 12 bytes, mypc.o(i.myPC_handle))
  [Stack]

  - Max Depth = 12
  - Call Chain = myPC_handle
  [Called By]
  - >> USER_Run

  myUSART_OverTime (Thumb, 16 bytes, Stack size 0 bytes, myuart.o(i.myUSART_OverTime))
  [Called By]

  - >> USER_Run

  ### Local Symbols

  DMA_CalcBaseAndBitshift (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal_dma.o(i.DMA_CalcBaseAndBitshift))
  [Stack]

  - Max Depth = 20
  - Call Chain = DMA_CalcBaseAndBitshift ⇒ __aeabi_uidivmod
  [Calls]
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_DMA_Init

  DMA_SetConfig (Thumb, 40 bytes, Stack size 12 bytes, stm32f0xx_hal_dma.o(i.DMA_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_SetConfig
  [Called By]
  - >> HAL_DMA_Start_IT

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f0xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_SlaveTimer_SetConfig (Thumb, 122 bytes, Stack size 16 bytes, stm32f0xx_hal_tim.o(i.TIM_SlaveTimer_SetConfig))
  [Stack]

  - Max Depth = 28
  - Call Chain = TIM_SlaveTimer_SetConfig ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> __ARM_common_switch8
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_SlaveConfigSynchronization

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 12 bytes, stm32f0xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource
  - >> TIM_SlaveTimer_SetConfig

  TIM_TI2_ConfigInputStage (Thumb, 38 bytes, Stack size 12 bytes, stm32f0xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource
  - >> TIM_SlaveTimer_SetConfig

  UART_DMAAbortOnError (Thumb, 20 bytes, Stack size 8 bytes, stm32f0xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMAAbortOnError ⇒ HAL_UART_ErrorCallback
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_EndRxTransfer (Thumb, 30 bytes, Stack size 0 bytes, stm32f0xx_hal_uart.o(i.UART_EndRxTransfer))
  [Called By]

  - >> HAL_UART_IRQHandler

  NVIC_SetPriority (Thumb, 60 bytes, Stack size 0 bytes, stm32f0xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_SYSTICK_Config
  - >> HAL_NVIC_SetPriority

  ADC_DMAConvCplt (Thumb, 108 bytes, Stack size 8 bytes, stm32f0xx_hal_adc.o(i.ADC_DMAConvCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DMAConvCplt
  [Calls]
  - >> HAL_ADC_ConvCpltCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA)

  ADC_DMAError (Thumb, 26 bytes, Stack size 8 bytes, stm32f0xx_hal_adc.o(i.ADC_DMAError))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DMAError
  [Calls]
  - >> HAL_ADC_ErrorCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA)

  ADC_DMAHalfConvCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32f0xx_hal_adc.o(i.ADC_DMAHalfConvCplt))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC_DMAHalfConvCplt
  [Calls]
  - >> HAL_ADC_ConvHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f0xx_hal_adc.o(i.HAL_ADC_Start_DMA)

  ADC_Enable (Thumb, 120 bytes, Stack size 24 bytes, stm32f0xx_hal_adc.o(i.ADC_Enable))
  [Stack]

  - Max Depth = 36
  - Call Chain = ADC_Enable ⇒ __aeabi_uidivmod
  [Calls]
  - >> HAL_GetTick
  - >> __aeabi_uidivmod
  [Called By]
  - >> HAL_ADC_Start_DMA

  ### Undefined Global Symbols