Protel Design System Design Rule Check
PCB File : E:\我的坚果云\【单片机】\【0我的工程】\【---数控电源3.0\A-底层驱动板\数控源9.8-竞赛开源\数控源-A9.8.PCBDOC
Date     : 2023/6/8
Time     : 14:58:28

Processing Rule : Hole Size Constraint (Min=0.0254mm) (Max=2.54mm) (All)
Rule Violations :0

Processing Rule : Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All)
Rule Violations :0

Processing Rule : Width Constraint (Min=0.2mm) (Max=2mm) (Preferred=0.3mm) (All)
Rule Violations :0

Processing Rule : Power Plane Connect Rule(Relief Connect )(Expansion=0.508mm) (Conductor Width=0.254mm) (Air Gap=0.254mm) (Entries=4) (All)
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.2mm) (All),(All)
   Violation between Pad Z-1(360.25mm,219.25mm)  Multi-Layer and 
                     Pad Z-0(360.25mm,219.25mm)  Bottom Layer
Rule Violations :1

Processing Rule : Broken-Net Constraint ( (All) )
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=No) (All),(All)
   Violation between Pad Z-0(358.65mm,216.65mm)  Multi-Layer and 
                     Pad Z-0(360.25mm,219.25mm)  Bottom Layer
   Violation between Pad Z-0(361.85mm,216.65mm)  Multi-Layer and 
                     Pad Z-0(360.25mm,219.25mm)  Bottom Layer
   Violation between Pad Z-0(358.65mm,221.85mm)  Multi-Layer and 
                     Pad Z-0(360.25mm,219.25mm)  Bottom Layer
   Violation between Pad Z-1(360.25mm,219.25mm)  Multi-Layer and 
                     Pad Z-0(360.25mm,219.25mm)  Bottom Layer
   Violation between Pad Z-0(361.85mm,221.85mm)  Multi-Layer and 
                     Pad Z-0(360.25mm,219.25mm)  Bottom Layer
Rule Violations :5


Violations Detected : 6
Time Elapsed        : 00:00:00