customize

# Design Rule Verification Report

Date | : | 2022-11-22
Time | : | 11:25:38
Elapsed Time | : | 00:00:00
Filename | : | E:\我的坚果云\【单片机】\【0我的工程】\【---数控电源3.0\C-面板\3.1版\数控源-C.PcbDoc

Warnings | : | 0
Rule Violations | : | 1

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Broken-Net Constraint ( (All) ) | 1
Clearance Constraint (Gap=0.2mm) (All),(All) | 0
Power Plane Connect Rule(Relief Connect )(Expansion=0.508mm) (Conductor Width=0.254mm) (Air Gap=0.254mm) (Entries=4) (All) | 0
Width Constraint (Min=0.2mm) (Max=2mm) (Preferred=0.4mm) (All) | 0
Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All) | 0
Hole Size Constraint (Min=0.0254mm) (Max=2.54mm) (All) | 0
Total | 1

Broken-Net Constraint ( (All) )
Net IRQ is broken into 2 sub-nets. Routed To 75.00% Subnet : S-14 IRQ2-1 Subnet : fpc1-10 b1116-14 IRQ1-1

Back to top